\hypertarget{structLCI__gemInput}{
\section{LCI\_\-gemInput Struct Reference}
\label{structLCI__gemInput}\index{LCI\_\-gemInput@{LCI\_\-gemInput}}
}
The GEM configuration parameters stored in binary file.  


{\tt \#include $<$configure\_\-p.h$>$}

\subsection*{Public Attributes}
\begin{CompactItemize}
\item 
\hypertarget{structLCI__gemInput_8a4ca68023f712a8f2ce999b642b45b3}{
unsigned \hyperlink{structLCI__gemInput_8a4ca68023f712a8f2ce999b642b45b3}{nev}}
\label{structLCI__gemInput_8a4ca68023f712a8f2ce999b642b45b3}

\begin{CompactList}\small\item\em Number of events to collect for each cycle performed using this configuration. \item\end{CompactList}\item 
\hypertarget{structLCI__gemInput_72a1edbc7f3b21eafa8ce7b01f427628}{
unsigned \hyperlink{structLCI__gemInput_72a1edbc7f3b21eafa8ce7b01f427628}{latcDelay}}
\label{structLCI__gemInput_72a1edbc7f3b21eafa8ce7b01f427628}

\begin{CompactList}\small\item\em Delay after changing the LATC configuration to allow for settling. \item\end{CompactList}\item 
\hypertarget{structLCI__gemInput_992a7161e3b27d17036b1a25423560fd}{
unsigned \hyperlink{structLCI__gemInput_992a7161e3b27d17036b1a25423560fd}{delay}}
\label{structLCI__gemInput_992a7161e3b27d17036b1a25423560fd}

\begin{CompactList}\small\item\em Delay after changing the inj DAC settings to allow for settling. \item\end{CompactList}\item 
\hypertarget{structLCI__gemInput_250df4915ac0d025c220fc712e3898e3}{
unsigned \hyperlink{structLCI__gemInput_250df4915ac0d025c220fc712e3898e3}{\_\-\_\-pad0\_\-\_\-}: 5}
\label{structLCI__gemInput_250df4915ac0d025c220fc712e3898e3}

\begin{CompactList}\small\item\em Padding. \item\end{CompactList}\item 
\hypertarget{structLCI__gemInput_212c0c8c9a84da0ee13c0e42718b11a6}{
unsigned \hyperlink{structLCI__gemInput_212c0c8c9a84da0ee13c0e42718b11a6}{one\_\-range}: 1}
\label{structLCI__gemInput_212c0c8c9a84da0ee13c0e42718b11a6}

\begin{CompactList}\small\item\em Use single-range readout, not 4-range. \item\end{CompactList}\item 
\hypertarget{structLCI__gemInput_31bb5247d60a827bd15e41863a363fcb}{
unsigned \hyperlink{structLCI__gemInput_31bb5247d60a827bd15e41863a363fcb}{zero\_\-suppress}: 1}
\label{structLCI__gemInput_31bb5247d60a827bd15e41863a363fcb}

\begin{CompactList}\small\item\em Zero suppress. \item\end{CompactList}\item 
\hypertarget{structLCI__gemInput_060d507fedec9a05860843821a807cd9}{
unsigned \hyperlink{structLCI__gemInput_060d507fedec9a05860843821a807cd9}{strobe}: 1}
\label{structLCI__gemInput_060d507fedec9a05860843821a807cd9}

\begin{CompactList}\small\item\em Send the CALSTROBE. \item\end{CompactList}\item 
\hypertarget{structLCI__gemInput_906ae575a65d5c673e07a65236f4f1ac}{
unsigned \hyperlink{structLCI__gemInput_906ae575a65d5c673e07a65236f4f1ac}{period}:24}
\label{structLCI__gemInput_906ae575a65d5c673e07a65236f4f1ac}

\begin{CompactList}\small\item\em Number of clock-ticks between events - reqd to be $>$= 20000 (for a 1khz max rate). \item\end{CompactList}\end{CompactItemize}


\subsection{Detailed Description}
The GEM configuration parameters stored in binary file. 

\begin{Desc}
\item[Warning:]This structure is written to and read from the filesystem so do not add elements that are are for internal use only \end{Desc}


The documentation for this struct was generated from the following file:\begin{CompactItemize}
\item 
\hyperlink{configure__p_8h}{configure\_\-p.h}\end{CompactItemize}
