\hypertarget{structLCI__gemInput}{
\section{LCI\_\-gem\-Input Struct Reference}
\label{structLCI__gemInput}\index{LCI_gemInput@{LCI\_\-gemInput}}
}
The GEM configuration parameters stored in binary file.  


{\tt \#include $<$configure\_\-p.h$>$}

\subsection*{Data Fields}
\begin{CompactItemize}
\item 
\hypertarget{structLCI__gemInput_o0}{
unsigned \hyperlink{structLCI__gemInput_o0}{nev}}
\label{structLCI__gemInput_o0}

\begin{CompactList}\small\item\em Number of events to collect for each cycle performed using this configuration. \item\end{CompactList}\item 
\hypertarget{structLCI__gemInput_o1}{
unsigned \hyperlink{structLCI__gemInput_o1}{latc\-Delay}}
\label{structLCI__gemInput_o1}

\begin{CompactList}\small\item\em Delay after changing the LATC configuration to allow for settling. \item\end{CompactList}\item 
\hypertarget{structLCI__gemInput_o2}{
unsigned \hyperlink{structLCI__gemInput_o2}{delay}}
\label{structLCI__gemInput_o2}

\begin{CompactList}\small\item\em Delay after changing the inj DAC settings to allow for settling. \item\end{CompactList}\item 
\hypertarget{structLCI__gemInput_o3}{
unsigned \hyperlink{structLCI__gemInput_o3}{\_\-\_\-pad0\_\-\_\-}: 5}
\label{structLCI__gemInput_o3}

\begin{CompactList}\small\item\em Padding. \item\end{CompactList}\item 
\hypertarget{structLCI__gemInput_o4}{
unsigned \hyperlink{structLCI__gemInput_o4}{auto\_\-range}: 1}
\label{structLCI__gemInput_o4}

\begin{CompactList}\small\item\em Do not use 4-range readout. \item\end{CompactList}\item 
\hypertarget{structLCI__gemInput_o5}{
unsigned \hyperlink{structLCI__gemInput_o5}{zero\_\-suppress}: 1}
\label{structLCI__gemInput_o5}

\begin{CompactList}\small\item\em Zero suppress. \item\end{CompactList}\item 
\hypertarget{structLCI__gemInput_o6}{
unsigned \hyperlink{structLCI__gemInput_o6}{strobe}: 1}
\label{structLCI__gemInput_o6}

\begin{CompactList}\small\item\em Send the CALSTROBE. \item\end{CompactList}\item 
\hypertarget{structLCI__gemInput_o7}{
unsigned \hyperlink{structLCI__gemInput_o7}{period}:24}
\label{structLCI__gemInput_o7}

\begin{CompactList}\small\item\em Number of clock-ticks between events - reqd to be $>$= 20000 (for a 1khz max rate). \item\end{CompactList}\end{CompactItemize}


\subsection{Detailed Description}
The GEM configuration parameters stored in binary file. 

\begin{Desc}
\item[Warning:]This structure is written to and read from the filesystem so do not add elements that are are for internal use only\end{Desc}




The documentation for this struct was generated from the following file:\begin{CompactItemize}
\item 
\hyperlink{configure__p_8h}{configure\_\-p.h}\end{CompactItemize}
