\hypertarget{interface_synopsis}{}\subsection{Synopsis}\label{synopsis}
{\tt lfs\_\-rt} - Test application for file uploads using Summit 1553 RT driver.\hypertarget{interface_description}{}\subsection{Description}\label{description}
This is a simple test application for GLAST 1553 file upload procedures. A small set of commands is provided to receive a file from the BC target machine across the 1553. The file upload command packets are processed, and target files are commited to storage at the application level in one of the RT target machine file systems. The names are always stored with the LAT file path naming convention, as determined by the file ID presented in the file upload commit command.

No telemetry is sent back from the RT.

The following commands are accepted from the shell once the test application is started: \par


{\tt  rt\_\-init \mbox{[}file\_\-size\mbox{]} } - Initialize the BC file upload application. The {\em file\_\-size\/} parameter sets the size in bytes of the largest file to be loaded. If no value is given, a 1 MB maximum upload size is set.\par
 {\tt  rt\_\-start } - Start listening on the 1553 bus . Spawns packet receive tasks. \par
 {\tt  rt\_\-stop } - Stop listening on the 1553 bus . Deletes packet receive tasks. \par
 {\tt  rt\_\-exit } - Shutdown test application. \par
 {\tt  rt\_\-info } - Display 1553 RT driver diagnostics. \par
 {\tt  upl\_\-info } - Display file upload state machine diagnostics. \par
