

\hypertarget{name}{}\subsection{Name}\label{name}


{\tt BIUDMP} - Dump a GLAST BFEM BIU housekeeping telemetry binary file into a comma delimeted text file.

\hypertarget{synopsis}{}\subsection{Synopsis}\label{synopsis}


{\tt   BIUDMP {\em  biu\_\-telemetry\_\-file } }

  \begin{TabularC}{2}
\hline
 biu\_\-telemetry\_\-file & The BIU binary telemetry log file to dump. \\\hline
\end{TabularC}


\hypertarget{description}{}\subsection{Description}\label{description}


The {\tt BIUDMP} application will extract values from a BIU telemetry log file recored by {\tt BIUCNSL} and display the values in text format suitable for use with Excel. The text dump is a comma delimited list of lines, with each line representing one second. The column definitions are listed below.

{\tt 

A - The BIU housekeeping packet sequence count (hex). \par
 B - The BIU UTC time for this packet. \par
 C - The total number of BIU telemetry frames transmitted. \par
 D - The current BIU telemetry transmit rate in bit / sec. \par
 E - The system 28V current. \par
 F - The system 28V voltage. \par
 G - The command interface 28V voltage. \par
 H - The command interface 28V current. \par
 I - The command interface 5V voltage. \par
 J - The XGT (fans) 12V voltage. \par
 K - The TKR base plate temperature. \par
 L - The pressure vessel upper air temperature. \par
 M - The DAQ 5V voltage. \par
 N - The DAQ 5V current. \par
 O - The DAQ +12V voltage. \par
 P - The DAQ +12V current. \par
 Q - The DAQ -12V voltage. \par
 R - The DAQ -12V current. \par
 S - The DAQ power supply temperature. \par
 T - The DAQ CPU temperature. \par
 U - The BIU 5V voltage. \par
 V - The BIU 5V current. \par
 W - The BIU +12V voltage. \par
 X - The BIU +12V current. \par
 Y - The BIU -12V voltage. \par
 Z - The BIU -12V current. \par
 AA - The BIU power supply temperature. \par
 AB - The pressure vessel lower air temperature. \par
 AC - The disk A 5V voltage. \par
 AD - The disk A 5V current. \par
 AE - The disk drive temperature. \par
 AF - The disk B 5V voltage. \par
 AG - The disk B 5V current. \par
 AH - The disk power supply temperature. \par
 AI - The pressure vessel bulkhead temperature. \par
 AJ - The pressure vessel radiator temperature. \par
 AK - The number of telemetry packets trasmitted in the last second. \par
 AL - The number of DAQ event packets received in the last second. \par
 AM - The number of DAQ event packets dropped in the last second. \par
 AN - The number of DAQ housekeeping packets received in the last second. \par
 AO - The total number of CIP commands received. \par
 AP - The total number of CIP command rejected. \par
 AQ - The total number of command forwarded to the DAQ. \par
 AR - The total number of BIU command executed. \par
 AS - The total number of BIU command errors. \par
 AT - The last BIU command word (hex). \par
 AU - The total number of BIU errors. \par
 AV - The last BIU error code. \par
 AW - The current BIU telemetry mode. \par
 AX - The BIU VME 5V voltage. \par
 AY - The BIU VME ground voltage. \par
 AZ - The external temperature \#0. \par
 BA - The external temperature \#1. \par
 BB - The external temperature \#2. \par
 BC - The external temperature \#3. \par
 BD - The external temperature \#4. \par


}

