

\hypertarget{synopsis}{}\subsection{Synopsis}\label{synopsis}


{\tt  BSET\_\-start {\em  task\_\-pri, task\_\-stack }, {\em  tx\_\-rate } }

  \begin{TabularC}{2}
\hline
 task\_\-pri & The priority of the BSET application task.  \\\hline
 task\_\-stack & The stack size of the BSET application task.  \\\hline
 tx\_\-rate & The initial telemetry rate in bits / sec. \\\hline
\end{TabularC}


\hypertarget{description}{}\subsection{Description}\label{description}


The {\tt BSET} application is a UDP/IP server which handles dynamically tuning the SBS 4400-VF10 Bit Synchronizer. The {\tt BSET} application listens on UDP port \hyperlink{BSET__port_8h_a0}{BSET\_\-RATE\_\-PORT} for bit rate set commands. Each command is simply a single 32-bit word giving the new bit rate.

