

\hypertarget{synopsis}{}\subsection{Synopsis}\label{synopsis}


{\tt   NSBFSIM {\em  a$|$b }  }

  \begin{TabularC}{2}
\hline
 a & Use serial port device /dev/ttya.  \\\hline
 b & Use serial port device /dev/ttyb. \\\hline
\end{TabularC}


\hypertarget{description}{}\subsection{Description}\label{description}


The {\tt NSBFSIM} application outputs a simulated NSBF GPS message on either serial port a or port b on Solaris machines. The GPS will be sent once every 10 seconds. The application does not simulate the reception of  commands from the BFEM command GSE.

