\hypertarget{structLCFG__controller}{
\section{LCFG\_\-controller Struct Reference}
\label{structLCFG__controller}\index{LCFG_controller@{LCFG\_\-controller}}
}
Structure used by LCFG to perform its duties.  


Collaboration diagram for LCFG\_\-controller:\begin{figure}[H]
\begin{center}
\leavevmode
\includegraphics[width=65pt]{structLCFG__controller__coll__graph}
\end{center}
\end{figure}
\subsection*{Data Fields}
\begin{CompactItemize}
\item 
\hypertarget{structLCFG__controller_o0}{
unsigned \hyperlink{structLCFG__controller_o0}{cache\-Fid}}
\label{structLCFG__controller_o0}

\begin{CompactList}\small\item\em The file ID of the LAT configuration master file used to create the current cached IMM. \item\end{CompactList}\item 
\hypertarget{structLCFG__controller_o1}{
unsigned \hyperlink{structLCFG__controller_o1}{ignore\-Fid}}
\label{structLCFG__controller_o1}

\begin{CompactList}\small\item\em The file ID of the LAT ignore file. \item\end{CompactList}\item 
\hypertarget{structLCFG__controller_o2}{
unsigned \hyperlink{structLCFG__controller_o2}{cache\-Key}}
\label{structLCFG__controller_o2}

\begin{CompactList}\small\item\em The file key of the LAT configuration master file used to create the current cached IMM. \item\end{CompactList}\item 
\hypertarget{structLCFG__controller_o3}{
unsigned \hyperlink{structLCFG__controller_o3}{config\-Key}}
\label{structLCFG__controller_o3}

\begin{CompactList}\small\item\em The file key of the LAT configuration master file used to create the last IMM that was used to configure the LAT. \item\end{CompactList}\item 
\hypertarget{structLCFG__controller_o4}{
unsigned \hyperlink{structLCFG__controller_o4}{ignore\-Key}}
\label{structLCFG__controller_o4}

\begin{CompactList}\small\item\em The file key of the LAT ignore file. \item\end{CompactList}\item 
\hypertarget{structLCFG__controller_o5}{
RIM $\ast$ \hyperlink{structLCFG__controller_o5}{cache}}
\label{structLCFG__controller_o5}

\begin{CompactList}\small\item\em The last configuration read from file and applied to the LAT. \item\end{CompactList}\item 
\hypertarget{structLCFG__controller_o6}{
RIM $\ast$ \hyperlink{structLCFG__controller_o6}{capture}}
\label{structLCFG__controller_o6}

\begin{CompactList}\small\item\em In-memory model of the current configuration of the LAT. \item\end{CompactList}\item 
\hypertarget{structLCFG__controller_o7}{
RIM\_\-map $\ast$ \hyperlink{structLCFG__controller_o7}{ignore}}
\label{structLCFG__controller_o7}

\begin{CompactList}\small\item\em Bit-map indicating the portions of the LAT to ignore during verification or capture. \item\end{CompactList}\item 
\hypertarget{structLCFG__controller_o8}{
\hyperlink{struct__LCFG__hsk}{LCFG\_\-hsk} $\ast$ \hyperlink{structLCFG__controller_o8}{hsk}}
\label{structLCFG__controller_o8}

\begin{CompactList}\small\item\em Address of LCFG housekeeping information. \item\end{CompactList}\item 
\hypertarget{structLCFG__controller_o9}{
FPA\_\-fcb $\ast$ \hyperlink{structLCFG__controller_o9}{fpa}}
\label{structLCFG__controller_o9}

\begin{CompactList}\small\item\em Fixed packet allocator that provide storage for the construction of datagrams sent to the SSR. \item\end{CompactList}\item 
\hypertarget{structLCFG__controller_o10}{
void $\ast$ \hyperlink{structLCFG__controller_o10}{buf}}
\label{structLCFG__controller_o10}

\begin{CompactList}\small\item\em Buffer associated with the FPA. \item\end{CompactList}\item 
\hypertarget{structLCFG__controller_o11}{
RIM\_\-load\-Fn $\ast$$\ast$ \hyperlink{structLCFG__controller_o11}{load}}
\label{structLCFG__controller_o11}

\begin{CompactList}\small\item\em Ordered array of function pointers linking register types and load functions. \item\end{CompactList}\item 
\hypertarget{structLCFG__controller_o12}{
RIM\_\-decode\-Fn $\ast$$\ast$ \hyperlink{structLCFG__controller_o12}{decode}}
\label{structLCFG__controller_o12}

\begin{CompactList}\small\item\em Ordered array of function pointers linking register types and decode functions. \item\end{CompactList}\item 
\hypertarget{structLCFG__controller_o13}{
RIM\_\-read\-Fn $\ast$$\ast$ \hyperlink{structLCFG__controller_o13}{read}}
\label{structLCFG__controller_o13}

\begin{CompactList}\small\item\em Ordered array of function pointers linking register types and read functions. \item\end{CompactList}\item 
\hypertarget{structLCFG__controller_o14}{
RIM\_\-rqst\-Info $\ast$ \hyperlink{structLCFG__controller_o14}{rqi}}
\label{structLCFG__controller_o14}

\begin{CompactList}\small\item\em Array of items accompanying a command list used to provide decode info. \item\end{CompactList}\item 
\hypertarget{structLCFG__controller_o15}{
LEM\_\-micr $\ast$ \hyperlink{structLCFG__controller_o15}{cr}}
\label{structLCFG__controller_o15}

\begin{CompactList}\small\item\em Multi-item command/response list used to interact with the LAT. \item\end{CompactList}\end{CompactItemize}


\subsection{Detailed Description}
Structure used by LCFG to perform its duties. 



The documentation for this struct was generated from the following file:\begin{CompactItemize}
\item 
\hyperlink{LCFG__lcfg_8c}{LCFG\_\-lcfg.c}\end{CompactItemize}
