\hypertarget{struct__HfcCfgCal}{
\section{\_\-HfcCfgCal Struct Reference}
\label{struct__HfcCfgCal}\index{\_\-HfcCfgCal@{\_\-HfcCfgCal}}
}
System control structure for the CAL cuts.  


{\tt \#include $<$HFC\_\-def.h$>$}

\subsection*{Public Attributes}
\begin{CompactItemize}
\item 
unsigned int \hyperlink{struct__HfcCfgCal_5f34635c8a6096b2a9bee33035eb1e4f}{ethreshold}
\item 
unsigned int \hyperlink{struct__HfcCfgCal_b3f5b34dfb0e846bbd508febbde7ae50}{nmaxlogs}
\item 
unsigned int \hyperlink{struct__HfcCfgCal_885e76ccb7345088756806b536d92cac}{tolerance}
\end{CompactItemize}


\subsection{Detailed Description}
System control structure for the CAL cuts. 

\subsection{Member Data Documentation}
\hypertarget{struct__HfcCfgCal_5f34635c8a6096b2a9bee33035eb1e4f}{
\index{\_\-HfcCfgCal@{\_\-HfcCfgCal}!ethreshold@{ethreshold}}
\index{ethreshold@{ethreshold}!_HfcCfgCal@{\_\-HfcCfgCal}}
\subsubsection[{ethreshold}]{\setlength{\rightskip}{0pt plus 5cm}unsigned int {\bf \_\-HfcCfgCal::ethreshold}}}
\label{struct__HfcCfgCal_5f34635c8a6096b2a9bee33035eb1e4f}


The threshold, in 2$\ast$LEU, to consider a log hit, The factor of 2 comes from adding each end. Typically 50 Mev =$>$ 400/ 

Referenced by cal\_\-check(), and compileCfgPrms().\hypertarget{struct__HfcCfgCal_b3f5b34dfb0e846bbd508febbde7ae50}{
\index{\_\-HfcCfgCal@{\_\-HfcCfgCal}!nmaxlogs@{nmaxlogs}}
\index{nmaxlogs@{nmaxlogs}!_HfcCfgCal@{\_\-HfcCfgCal}}
\subsubsection[{nmaxlogs}]{\setlength{\rightskip}{0pt plus 5cm}unsigned int {\bf \_\-HfcCfgCal::nmaxlogs}}}
\label{struct__HfcCfgCal_b3f5b34dfb0e846bbd508febbde7ae50}


The maximum number of logs per layer that can be above the the energy threshold, typically, 2. 

Referenced by cal\_\-check(), and compileCfgPrms().\hypertarget{struct__HfcCfgCal_885e76ccb7345088756806b536d92cac}{
\index{\_\-HfcCfgCal@{\_\-HfcCfgCal}!tolerance@{tolerance}}
\index{tolerance@{tolerance}!_HfcCfgCal@{\_\-HfcCfgCal}}
\subsubsection[{tolerance}]{\setlength{\rightskip}{0pt plus 5cm}unsigned int {\bf \_\-HfcCfgCal::tolerance}}}
\label{struct__HfcCfgCal_885e76ccb7345088756806b536d92cac}


The layer-to-layer tolerance, typically 50\%, this is expressed in units of 128, so 1 $\sim$= $\sim$1\%. Typically 30\% 

Referenced by cal\_\-check(), and compileCfgPrms().

The documentation for this struct was generated from the following file:\begin{CompactItemize}
\item 
\hyperlink{HFC__def_8h}{HFC\_\-def.h}\end{CompactItemize}
