\hypertarget{interface_description}{}\subsection{Description}\label{interface_description}
The qcfg\_\-print program is used to display the contents of a file of LAT configuration datagrams sent from the instrument. Each datagram contains a complete set of binary configuration data recorded by reading the instrument's registers. By default the first datagram in the file is displayed, but options exist to display any one datagram, or all.\hypertarget{interface_synopsis}{}\subsection{Synopsis}\label{interface_synopsis}
\begin{TabularC}{2}
\hline
qcfg\_\-print &\mbox{[}-v\mbox{]} \mbox{[}-s\mbox{]} \mbox{[}-a\mbox{]} \mbox{[}-x\mbox{]} \mbox{[}-i index\mbox{]} \mbox{[}-x out\-File\mbox{]} dgm\-File  \\\hline
\end{TabularC}
\hypertarget{interface_options}{}\subsection{Options}\label{interface_options}
\begin{TabularC}{2}
\hline
-o~{\em out\-File\/}  &The name of the output file to receive the generated report.  \\\hline
-i~{\em index\/} 

&Causes the {\em index\/} datagram in the file to be displayed. The default is 1.  \\\hline
-x &Causes XML source to be generated instead of a report.  \\\hline
-a &Causes all datagrams in the file to be displayed in sequence.  \\\hline
-v &Verbose option. Causes a summary line showing the number of datagrams processed to be displayed at the end.  \\\hline
-s &Causes only the summary line to be displayed.  \\\hline
\end{TabularC}
\hypertarget{interface_parameters}{}\subsection{Parameters}\label{interface_parameters}
\begin{TabularC}{2}
\hline
{\em dgm\-File\/}  &The name of the configuration datagram file to read.  \\\hline
\end{TabularC}
