\hypertarget{MEMCMD_8h}{
\section{MEMCMD.h File Reference}
\label{MEMCMD_8h}\index{MEMCMD.h@{MEMCMD.h}}
}
 


{\tt \#include \char`\"{}MEM/MEM\_\-apid.h\char`\"{}}\par
{\tt \#include \char`\"{}MEM/MEM\_\-cmddefs.h\char`\"{}}\par


Include dependency graph for MEMCMD.h:\begin{figure}[H]
\begin{center}
\leavevmode
\includegraphics[width=147pt]{MEMCMD_8h__incl}
\end{center}
\end{figure}


This graph shows which files directly or indirectly include this file:\begin{figure}[H]
\begin{center}
\leavevmode
\includegraphics[width=144pt]{MEMCMD_8h__dep__incl}
\end{center}
\end{figure}
\subsection*{Defines}
\begin{CompactItemize}
\item 
\#define \hyperlink{MEMCMD_8h_a0}{MEM\_\-APID\_\-LAT\_\-MEM\_\-LOAD}\ (MEM\_\-APID\_\-CMD\_\-DUMP\_\-LOAD)
\item 
\#define \hyperlink{MEMCMD_8h_a1}{MEM\_\-FC\_\-MEM\_\-LOAD\_\-MEMORY}\ (4)
\item 
\#define \hyperlink{MEMCMD_8h_a2}{MEM\_\-FC\_\-MEM\_\-LOAD\_\-PCI}\ (5)
\item 
\#define \hyperlink{MEMCMD_8h_a3}{MEM\_\-FC\_\-MEM\_\-LOAD\_\-REGISTER}\ (6)
\item 
\#define \hyperlink{MEMCMD_8h_a4}{MEM\_\-APID\_\-LAT\_\-MEM\_\-DUMP}\ (MEM\_\-APID\_\-CMD\_\-DUMP\_\-LOAD)
\item 
\#define \hyperlink{MEMCMD_8h_a5}{MEM\_\-FC\_\-MEM\_\-DUMP\_\-MEMORY}\ (0)
\item 
\#define \hyperlink{MEMCMD_8h_a6}{MEM\_\-FC\_\-MEM\_\-DUMP\_\-CANCEL}\ (1)
\item 
\#define \hyperlink{MEMCMD_8h_a7}{MEM\_\-FC\_\-MEM\_\-DUMP\_\-PCI}\ (2)
\item 
\#define \hyperlink{MEMCMD_8h_a8}{MEM\_\-FC\_\-MEM\_\-DUMP\_\-REGISTER}\ (3)
\end{CompactItemize}


\subsection{Detailed Description}
\begin{Desc}
\item[Author:]Ray Caperoon \end{Desc}
\begin{Desc}
\item[Date:]Fri Sep 26 09:23:13 2003\end{Desc}
Placeholder for memory commands from CTDB.

\begin{Desc}
\item[Date]2004/11/19 19:35:59 \end{Desc}
\begin{Desc}
\item[Source]/nfs/slac/g/glast/flight/archive/MEM/MEM/MEMCMD.h,v \end{Desc}
\begin{Desc}
\item[Author]dmay \end{Desc}
\begin{Desc}
\item[Revision]1.7 \end{Desc}
\begin{Desc}
\item[Log]\hyperlink{MEMCMD_8h}{MEMCMD.h},v \end{Desc}
Revision 1.7 2004/11/19 19:35:59 dmay use \hyperlink{MEM__apid_8h}{MEM\_\-apid.h}

Revision 1.6 2004/07/23 16:30:23 dmay merge APIDs; reallocate function codes; add 'len' param to ITC callbacks

Revision 1.5 2004/07/19 16:06:26 dmay include definitions produced by LCAT

Revision 1.4 2004/06/17 20:01:20 dmay increase max load words from 11 to 1024

Revision 1.3 2004/05/03 20:21:37 dmay Added MEM\_\-LOAD\_\-MEMORY\_\-MAX\_\-WORDS; Added lat\-Unit to the Dump\-Register command

Revision 1.2 2004/03/09 13:41:48 ray added LAT unit to commands, removed old command defs

Revision 1.1.1.1 2004/01/09 12:52:27 ray Create package MEM

\subsection{Define Documentation}
\hypertarget{MEMCMD_8h_a4}{
\index{MEMCMD.h@{MEMCMD.h}!MEM_APID_LAT_MEM_DUMP@{MEM\_\-APID\_\-LAT\_\-MEM\_\-DUMP}}
\index{MEM_APID_LAT_MEM_DUMP@{MEM\_\-APID\_\-LAT\_\-MEM\_\-DUMP}!MEMCMD.h@{MEMCMD.h}}
\subsubsection[MEM\_\-APID\_\-LAT\_\-MEM\_\-DUMP]{\setlength{\rightskip}{0pt plus 5cm}\#define MEM\_\-APID\_\-LAT\_\-MEM\_\-DUMP\ (MEM\_\-APID\_\-CMD\_\-DUMP\_\-LOAD)}}
\label{MEMCMD_8h_a4}


APID for memory dump telecommands. \hypertarget{MEMCMD_8h_a0}{
\index{MEMCMD.h@{MEMCMD.h}!MEM_APID_LAT_MEM_LOAD@{MEM\_\-APID\_\-LAT\_\-MEM\_\-LOAD}}
\index{MEM_APID_LAT_MEM_LOAD@{MEM\_\-APID\_\-LAT\_\-MEM\_\-LOAD}!MEMCMD.h@{MEMCMD.h}}
\subsubsection[MEM\_\-APID\_\-LAT\_\-MEM\_\-LOAD]{\setlength{\rightskip}{0pt plus 5cm}\#define MEM\_\-APID\_\-LAT\_\-MEM\_\-LOAD\ (MEM\_\-APID\_\-CMD\_\-DUMP\_\-LOAD)}}
\label{MEMCMD_8h_a0}


APID for memory load telecommands. \hypertarget{MEMCMD_8h_a6}{
\index{MEMCMD.h@{MEMCMD.h}!MEM_FC_MEM_DUMP_CANCEL@{MEM\_\-FC\_\-MEM\_\-DUMP\_\-CANCEL}}
\index{MEM_FC_MEM_DUMP_CANCEL@{MEM\_\-FC\_\-MEM\_\-DUMP\_\-CANCEL}!MEMCMD.h@{MEMCMD.h}}
\subsubsection[MEM\_\-FC\_\-MEM\_\-DUMP\_\-CANCEL]{\setlength{\rightskip}{0pt plus 5cm}\#define MEM\_\-FC\_\-MEM\_\-DUMP\_\-CANCEL\ (1)}}
\label{MEMCMD_8h_a6}


Function code to indicate memory dump cancel telecommand. \hypertarget{MEMCMD_8h_a5}{
\index{MEMCMD.h@{MEMCMD.h}!MEM_FC_MEM_DUMP_MEMORY@{MEM\_\-FC\_\-MEM\_\-DUMP\_\-MEMORY}}
\index{MEM_FC_MEM_DUMP_MEMORY@{MEM\_\-FC\_\-MEM\_\-DUMP\_\-MEMORY}!MEMCMD.h@{MEMCMD.h}}
\subsubsection[MEM\_\-FC\_\-MEM\_\-DUMP\_\-MEMORY]{\setlength{\rightskip}{0pt plus 5cm}\#define MEM\_\-FC\_\-MEM\_\-DUMP\_\-MEMORY\ (0)}}
\label{MEMCMD_8h_a5}


Function code to indicate memory dump register telecommand. \hypertarget{MEMCMD_8h_a7}{
\index{MEMCMD.h@{MEMCMD.h}!MEM_FC_MEM_DUMP_PCI@{MEM\_\-FC\_\-MEM\_\-DUMP\_\-PCI}}
\index{MEM_FC_MEM_DUMP_PCI@{MEM\_\-FC\_\-MEM\_\-DUMP\_\-PCI}!MEMCMD.h@{MEMCMD.h}}
\subsubsection[MEM\_\-FC\_\-MEM\_\-DUMP\_\-PCI]{\setlength{\rightskip}{0pt plus 5cm}\#define MEM\_\-FC\_\-MEM\_\-DUMP\_\-PCI\ (2)}}
\label{MEMCMD_8h_a7}


Function code to indicate memory dump PCI telecommand. \hypertarget{MEMCMD_8h_a8}{
\index{MEMCMD.h@{MEMCMD.h}!MEM_FC_MEM_DUMP_REGISTER@{MEM\_\-FC\_\-MEM\_\-DUMP\_\-REGISTER}}
\index{MEM_FC_MEM_DUMP_REGISTER@{MEM\_\-FC\_\-MEM\_\-DUMP\_\-REGISTER}!MEMCMD.h@{MEMCMD.h}}
\subsubsection[MEM\_\-FC\_\-MEM\_\-DUMP\_\-REGISTER]{\setlength{\rightskip}{0pt plus 5cm}\#define MEM\_\-FC\_\-MEM\_\-DUMP\_\-REGISTER\ (3)}}
\label{MEMCMD_8h_a8}


Function code to indicate memory dump register telecommand. \hypertarget{MEMCMD_8h_a1}{
\index{MEMCMD.h@{MEMCMD.h}!MEM_FC_MEM_LOAD_MEMORY@{MEM\_\-FC\_\-MEM\_\-LOAD\_\-MEMORY}}
\index{MEM_FC_MEM_LOAD_MEMORY@{MEM\_\-FC\_\-MEM\_\-LOAD\_\-MEMORY}!MEMCMD.h@{MEMCMD.h}}
\subsubsection[MEM\_\-FC\_\-MEM\_\-LOAD\_\-MEMORY]{\setlength{\rightskip}{0pt plus 5cm}\#define MEM\_\-FC\_\-MEM\_\-LOAD\_\-MEMORY\ (4)}}
\label{MEMCMD_8h_a1}


Function code to indicate memory load memory telecommand. \hypertarget{MEMCMD_8h_a2}{
\index{MEMCMD.h@{MEMCMD.h}!MEM_FC_MEM_LOAD_PCI@{MEM\_\-FC\_\-MEM\_\-LOAD\_\-PCI}}
\index{MEM_FC_MEM_LOAD_PCI@{MEM\_\-FC\_\-MEM\_\-LOAD\_\-PCI}!MEMCMD.h@{MEMCMD.h}}
\subsubsection[MEM\_\-FC\_\-MEM\_\-LOAD\_\-PCI]{\setlength{\rightskip}{0pt plus 5cm}\#define MEM\_\-FC\_\-MEM\_\-LOAD\_\-PCI\ (5)}}
\label{MEMCMD_8h_a2}


Function code to indicate memory load PCI telecommand. \hypertarget{MEMCMD_8h_a3}{
\index{MEMCMD.h@{MEMCMD.h}!MEM_FC_MEM_LOAD_REGISTER@{MEM\_\-FC\_\-MEM\_\-LOAD\_\-REGISTER}}
\index{MEM_FC_MEM_LOAD_REGISTER@{MEM\_\-FC\_\-MEM\_\-LOAD\_\-REGISTER}!MEMCMD.h@{MEMCMD.h}}
\subsubsection[MEM\_\-FC\_\-MEM\_\-LOAD\_\-REGISTER]{\setlength{\rightskip}{0pt plus 5cm}\#define MEM\_\-FC\_\-MEM\_\-LOAD\_\-REGISTER\ (6)}}
\label{MEMCMD_8h_a3}


Function code to indicate memory load register telecommand. 