\hypertarget{gGEMIE_8h}{
\section{g\-GEMIE.h File Reference}
\label{gGEMIE_8h}\index{gGEMIE.h@{gGEMIE.h}}
}
command/response methods for the GEM Input Enable register block  


{\tt \#include \char`\"{}GDAB/gdab.h\char`\"{}}\par
{\tt \#include \char`\"{}GDAB/ggem\_\-structs.h\char`\"{}}\par
\subsection*{Functions}
\begin{CompactItemize}
\item 
int \hyperlink{gGEMIE_8h_a0}{g\-GEMIEload} (\hyperlink{struct__gdab}{gdab\-Handle} gdab, unsigned short reg\-Id, \hyperlink{struct__gemIE}{gem\-IEHandle} val)
\begin{CompactList}\small\item\em Loads a register with value. \item\end{CompactList}\item 
int \hyperlink{gGEMIE_8h_a1}{g\-GEMIEread} (\hyperlink{struct__gdab}{gdab\-Handle} gdab, unsigned short reg\-Id, \hyperlink{struct__gemIE}{gem\-IEHandle} val)
\begin{CompactList}\small\item\em Reads a register returing value in {\em val\/}. \item\end{CompactList}\end{CompactItemize}


\subsection{Detailed Description}
command/response methods for the GEM Input Enable register block 

\begin{Desc}
\item[Author:]James Swain - \href{mailto:jswain@slac.stanford.edu}{\tt jswain@slac.stanford.edu}\end{Desc}


\subsection{Function Documentation}
\hypertarget{gGEMIE_8h_a0}{
\index{gGEMIE.h@{g\-GEMIE.h}!gGEMIEload@{gGEMIEload}}
\index{gGEMIEload@{gGEMIEload}!gGEMIE.h@{g\-GEMIE.h}}
\subsubsection[gGEMIEload]{\setlength{\rightskip}{0pt plus 5cm}int g\-GEMIEload (\hyperlink{struct__gdab}{gdab\-Handle} {\em gdab}, unsigned short {\em reg}, \hyperlink{struct__gemIE}{gem\-IEHandle} {\em value})}}
\label{gGEMIE_8h_a0}


Loads a register with value. 

\begin{Desc}
\item[Parameters:]
\begin{description}
\item[{\em gdab}]gdab\-Handle containing the COM I/O (gnat) handle \item[{\em reg}]register to load \item[{\em value}]64-bit value to load \end{description}
\end{Desc}
\begin{Desc}
\item[Returns:]G\_\-OK on success\end{Desc}
Loads the register {\em reg\/} from the the GEM Input Enable block with {\em value\/} \hypertarget{gGEMIE_8h_a1}{
\index{gGEMIE.h@{g\-GEMIE.h}!gGEMIEread@{gGEMIEread}}
\index{gGEMIEread@{gGEMIEread}!gGEMIE.h@{g\-GEMIE.h}}
\subsubsection[gGEMIEread]{\setlength{\rightskip}{0pt plus 5cm}int g\-GEMIEread (\hyperlink{struct__gdab}{gdab\-Handle} {\em gdab}, unsigned short {\em reg}, \hyperlink{struct__gemIE}{gem\-IEHandle} {\em value})}}
\label{gGEMIE_8h_a1}


Reads a register returing value in {\em val\/}. 

\begin{Desc}
\item[Parameters:]
\begin{description}
\item[{\em gdab}]gdab\-Handle containing the COM I/O (gnat) handle \item[{\em reg}]register to read \item[{\em value}]pointer to storage to hold the response of the read command \end{description}
\end{Desc}
\begin{Desc}
\item[Returns:]G\_\-OK on success\end{Desc}
Reads the register {\em reg\/} from the GEM Input Enable block. {\em val\/} is filled on return.

The following error codes are returned when LATp errors occur:

\begin{itemize}
\item GERR\_\-LATP\_\-HEADER\_\-PARITY \item GERR\_\-LATP\_\-CELL\_\-PARITY \item GERR\_\-LATP\_\-TRUNCATE \end{itemize}
