\section{Data Structures}
Here are the data structures with brief descriptions:\begin{CompactList}
\item\contentsline{section}{\hyperlink{struct____BFcellHeader}{\_\-\_\-BFcell\-Header} (Layout of a control cell header )}{\pageref{struct____BFcellHeader}}{}
\item\contentsline{section}{\hyperlink{union____cellHeader}{\_\-\_\-cell\-Header} (Union for 16-bit control cell header )}{\pageref{union____cellHeader}}{}
\item\contentsline{section}{\hyperlink{struct__BFregControl}{\_\-BFreg\-Control} (Map of the comm i/o board 32-bit control register )}{\pageref{struct__BFregControl}}{}
\item\contentsline{section}{\hyperlink{struct__BFregInt}{\_\-BFreg\-Int} (Map of the comm i/o board 32-bit interrupt config register )}{\pageref{struct__BFregInt}}{}
\item\contentsline{section}{\hyperlink{struct__BFregPF}{\_\-BFreg\-PF} (Map of the comm i/o board 32-bit playback FIFO register )}{\pageref{struct__BFregPF}}{}
\item\contentsline{section}{\hyperlink{struct__BFregRF}{\_\-BFreg\-RF} (Map of the comm i/o board 32-bit record FIFO register )}{\pageref{struct__BFregRF}}{}
\item\contentsline{section}{\hyperlink{struct__BFregStatus}{\_\-BFreg\-Status} (Map of the comm i/o board 32-bit status register )}{\pageref{struct__BFregStatus}}{}
\item\contentsline{section}{\hyperlink{struct__BFrspErr}{\_\-BFrsp\-Err} (Contains error info regarding LATp responses )}{\pageref{struct__BFrspErr}}{}
\item\contentsline{section}{\hyperlink{struct__BFtrgMsg}{\_\-BFtrg\-Msg} (Bit field definitions for a 32-bit trigger message )}{\pageref{struct__BFtrgMsg}}{}
\item\contentsline{section}{\hyperlink{struct__BFvasu__regEvtNum}{\_\-BFvasu\_\-reg\-Evt\-Num} (Map of the 32-bit event number register )}{\pageref{struct__BFvasu__regEvtNum}}{}
\item\contentsline{section}{\hyperlink{struct__BFvasu__regTestFeature}{\_\-BFvasu\_\-reg\-Test\-Feature} (Map of the VME vasu 32-bit test features register )}{\pageref{struct__BFvasu__regTestFeature}}{}
\item\contentsline{section}{\hyperlink{struct__BFvasu__regTrgCounter}{\_\-BFvasu\_\-reg\-Trg\-Counter} (Map of the VME vasu 32-bit trigger counter register )}{\pageref{struct__BFvasu__regTrgCounter}}{}
\item\contentsline{section}{\hyperlink{struct__BFvasu__regTrgMsg}{\_\-BFvasu\_\-reg\-Trg\-Msg} (Map of the VME vasu 32-bit trigger message register )}{\pageref{struct__BFvasu__regTrgMsg}}{}
\item\contentsline{section}{\hyperlink{struct__BFvasu__regTrgSequence}{\_\-BFvasu\_\-reg\-Trg\-Sequence} (Map of the VME vasu 32-bit trigger sequencing register )}{\pageref{struct__BFvasu__regTrgSequence}}{}
\item\contentsline{section}{\hyperlink{struct__BFvasu__regTrgSrc}{\_\-BFvasu\_\-reg\-Trg\-Src} (Map of the VME vasu 32-bit trigger source register )}{\pageref{struct__BFvasu__regTrgSrc}}{}
\item\contentsline{section}{\hyperlink{struct__driverInfo}{\_\-driver\-Info} (Common attributes about the driver version )}{\pageref{struct__driverInfo}}{}
\item\contentsline{section}{\hyperlink{union__generic__Cell}{\_\-generic\_\-Cell} (Union for 128-bit LATp cell -- either control or data cell )}{\pageref{union__generic__Cell}}{}
\item\contentsline{section}{\hyperlink{struct__gnat}{\_\-gnat} (Struct containing base parameters for the comm io board )}{\pageref{struct__gnat}}{}
\item\contentsline{section}{\hyperlink{struct__gResponse}{\_\-g\-Response} (Contains info for LATp responses )}{\pageref{struct__gResponse}}{}
\item\contentsline{section}{\hyperlink{struct__hardwareInfo}{\_\-hardware\-Info} (Attributes for the hardware configuration )}{\pageref{struct__hardwareInfo}}{}
\item\contentsline{section}{\hyperlink{struct__LATp__Cell}{\_\-LATp\_\-Cell} (LATp cell structure )}{\pageref{struct__LATp__Cell}}{}
\item\contentsline{section}{\hyperlink{struct__LATp__ControlCell}{\_\-LATp\_\-Control\-Cell} (Layout of a 128-bit LATp control cell )}{\pageref{struct__LATp__ControlCell}}{}
\item\contentsline{section}{\hyperlink{struct__LATp__DataCell}{\_\-LATp\_\-Data\-Cell} (Layout of a 128-bit LATp data cell )}{\pageref{struct__LATp__DataCell}}{}
\item\contentsline{section}{\hyperlink{struct__LATp__Interface}{\_\-LATp\_\-Interface} (Structure that defines a LATp interface )}{\pageref{struct__LATp__Interface}}{}
\item\contentsline{section}{\hyperlink{union__LATp__RXstats}{\_\-LATp\_\-RXstats} (Union for 16-bit LATp receiver statistics word )}{\pageref{union__LATp__RXstats}}{}
\item\contentsline{section}{\hyperlink{struct__LATp__RXstatsBF}{\_\-LATp\_\-RXstats\-BF} (Structure that defines the LATp receiver statistics word )}{\pageref{struct__LATp__RXstatsBF}}{}
\item\contentsline{section}{\hyperlink{union__LATp__TXstats}{\_\-LATp\_\-TXstats} (Union for 16-bit LATp transmitter statistics word )}{\pageref{union__LATp__TXstats}}{}
\item\contentsline{section}{\hyperlink{struct__LATp__TXstatsBF}{\_\-LATp\_\-TXstats\-BF} (Structure that defines the LATp transmitter statistics word )}{\pageref{struct__LATp__TXstatsBF}}{}
\item\contentsline{section}{\hyperlink{struct__regBlock}{\_\-reg\-Block} (Layout of COMM board register block )}{\pageref{struct__regBlock}}{}
\item\contentsline{section}{\hyperlink{union__regControl}{\_\-reg\-Control} (Union for 32-bit control register )}{\pageref{union__regControl}}{}
\item\contentsline{section}{\hyperlink{union__regInt}{\_\-reg\-Int} (Union for 32-bit interrupt register )}{\pageref{union__regInt}}{}
\item\contentsline{section}{\hyperlink{union__regPF}{\_\-reg\-PF} (Union for 32-bit play back FIFO register )}{\pageref{union__regPF}}{}
\item\contentsline{section}{\hyperlink{union__regRF}{\_\-reg\-RF} (Union for 32-bit record FIFO register )}{\pageref{union__regRF}}{}
\item\contentsline{section}{\hyperlink{union__regStatus}{\_\-reg\-Status} (Union for 32-bit status register )}{\pageref{union__regStatus}}{}
\item\contentsline{section}{\hyperlink{union__rspErr}{\_\-rsp\-Err} (Union for 32-bit response error flags )}{\pageref{union__rspErr}}{}
\item\contentsline{section}{\hyperlink{struct__sLog}{\_\-s\-Log} (Structure containing private parameters for logging objects )}{\pageref{struct__sLog}}{}
\item\contentsline{section}{\hyperlink{union__trgMsg}{\_\-trg\-Msg} (Union for 32-bit trigger message )}{\pageref{union__trgMsg}}{}
\item\contentsline{section}{\hyperlink{union__vasu__regEvtNum}{\_\-vasu\_\-reg\-Evt\-Num} (Union for 32-bit register )}{\pageref{union__vasu__regEvtNum}}{}
\item\contentsline{section}{\hyperlink{union__vasu__regTestFeature}{\_\-vasu\_\-reg\-Test\-Feature} (Union for 32-bit register )}{\pageref{union__vasu__regTestFeature}}{}
\item\contentsline{section}{\hyperlink{union__vasu__regTrgCounter}{\_\-vasu\_\-reg\-Trg\-Counter} (Union for 32-bit register )}{\pageref{union__vasu__regTrgCounter}}{}
\item\contentsline{section}{\hyperlink{union__vasu__regTrgMsg}{\_\-vasu\_\-reg\-Trg\-Msg} (Union for 32-bit register )}{\pageref{union__vasu__regTrgMsg}}{}
\item\contentsline{section}{\hyperlink{union__vasu__regTrgSequence}{\_\-vasu\_\-reg\-Trg\-Sequence} (Union for 32-bit register )}{\pageref{union__vasu__regTrgSequence}}{}
\item\contentsline{section}{\hyperlink{union__vasu__regTrgSrc}{\_\-vasu\_\-reg\-Trg\-Src} (Union for 32-bit register )}{\pageref{union__vasu__regTrgSrc}}{}
\item\contentsline{section}{\hyperlink{struct__vasuRegBlock}{\_\-vasu\-Reg\-Block} (Register Block for VASU )}{\pageref{struct__vasuRegBlock}}{}
\end{CompactList}
