\hypertarget{struct__regBlock}{
\section{\_\-reg\-Block Struct Reference}
\label{struct__regBlock}\index{_regBlock@{\_\-regBlock}}
}
layout of COMM board register block  


{\tt \#include $<$reg\_\-p.h$>$}

\subsection*{Data Fields}
\begin{CompactItemize}
\item 
volatile unsigned int \hyperlink{struct__regBlock_o0}{m\_\-ctrl\-Reg}
\item 
volatile unsigned int \hyperlink{struct__regBlock_o1}{m\_\-stat\-Reg}
\item 
volatile unsigned int \hyperlink{struct__regBlock_o2}{m\_\-pf\-Reg}
\item 
volatile unsigned int \hyperlink{struct__regBlock_o3}{m\_\-rf\-Reg}
\item 
volatile unsigned int \hyperlink{struct__regBlock_o4}{m\_\-int\-Reg}
\item 
volatile unsigned int \hyperlink{struct__regBlock_o5}{m\_\-mask\-Cfg\-Reg}
\item 
volatile unsigned int \hyperlink{struct__regBlock_o6}{m\_\-opt\-Reg}
\item 
volatile unsigned int \hyperlink{struct__regBlock_o7}{m\_\-trg\-Reg}
\end{CompactItemize}


\subsection{Detailed Description}
layout of COMM board register block 



\subsection{Field Documentation}
\hypertarget{struct__regBlock_o0}{
\index{_regBlock@{\_\-reg\-Block}!m_ctrlReg@{m\_\-ctrlReg}}
\index{m_ctrlReg@{m\_\-ctrlReg}!_regBlock@{\_\-reg\-Block}}
\subsubsection[m\_\-ctrlReg]{\setlength{\rightskip}{0pt plus 5cm}volatile unsigned int \hyperlink{struct__regBlock_o0}{\_\-reg\-Block::m\_\-ctrl\-Reg}}}
\label{struct__regBlock_o0}


comm i/o board control register, base addr + 0x00 \hypertarget{struct__regBlock_o4}{
\index{_regBlock@{\_\-reg\-Block}!m_intReg@{m\_\-intReg}}
\index{m_intReg@{m\_\-intReg}!_regBlock@{\_\-reg\-Block}}
\subsubsection[m\_\-intReg]{\setlength{\rightskip}{0pt plus 5cm}volatile unsigned int \hyperlink{struct__regBlock_o4}{\_\-reg\-Block::m\_\-int\-Reg}}}
\label{struct__regBlock_o4}


comm i/o board interrupt cfg register, base addr + 0x10 \hypertarget{struct__regBlock_o5}{
\index{_regBlock@{\_\-reg\-Block}!m_maskCfgReg@{m\_\-maskCfgReg}}
\index{m_maskCfgReg@{m\_\-maskCfgReg}!_regBlock@{\_\-reg\-Block}}
\subsubsection[m\_\-maskCfgReg]{\setlength{\rightskip}{0pt plus 5cm}volatile unsigned int \hyperlink{struct__regBlock_o5}{\_\-reg\-Block::m\_\-mask\-Cfg\-Reg}}}
\label{struct__regBlock_o5}


comm i/o board trg mask/cfg register, base addr + 0x14 \hypertarget{struct__regBlock_o6}{
\index{_regBlock@{\_\-reg\-Block}!m_optReg@{m\_\-optReg}}
\index{m_optReg@{m\_\-optReg}!_regBlock@{\_\-reg\-Block}}
\subsubsection[m\_\-optReg]{\setlength{\rightskip}{0pt plus 5cm}volatile unsigned int \hyperlink{struct__regBlock_o6}{\_\-reg\-Block::m\_\-opt\-Reg}}}
\label{struct__regBlock_o6}


comm i/o board trg options register, base addr + 0x18 \hypertarget{struct__regBlock_o2}{
\index{_regBlock@{\_\-reg\-Block}!m_pfReg@{m\_\-pfReg}}
\index{m_pfReg@{m\_\-pfReg}!_regBlock@{\_\-reg\-Block}}
\subsubsection[m\_\-pfReg]{\setlength{\rightskip}{0pt plus 5cm}volatile unsigned int \hyperlink{struct__regBlock_o2}{\_\-reg\-Block::m\_\-pf\-Reg}}}
\label{struct__regBlock_o2}


comm i/o board playback FIFO register, base addr + 0x08 \hypertarget{struct__regBlock_o3}{
\index{_regBlock@{\_\-reg\-Block}!m_rfReg@{m\_\-rfReg}}
\index{m_rfReg@{m\_\-rfReg}!_regBlock@{\_\-reg\-Block}}
\subsubsection[m\_\-rfReg]{\setlength{\rightskip}{0pt plus 5cm}volatile unsigned int \hyperlink{struct__regBlock_o3}{\_\-reg\-Block::m\_\-rf\-Reg}}}
\label{struct__regBlock_o3}


comm i/o board record FIFO register, base addr + 0x0C \hypertarget{struct__regBlock_o1}{
\index{_regBlock@{\_\-reg\-Block}!m_statReg@{m\_\-statReg}}
\index{m_statReg@{m\_\-statReg}!_regBlock@{\_\-reg\-Block}}
\subsubsection[m\_\-statReg]{\setlength{\rightskip}{0pt plus 5cm}volatile unsigned int \hyperlink{struct__regBlock_o1}{\_\-reg\-Block::m\_\-stat\-Reg}}}
\label{struct__regBlock_o1}


comm i/o board status register, base addr + 0x04 \hypertarget{struct__regBlock_o7}{
\index{_regBlock@{\_\-reg\-Block}!m_trgReg@{m\_\-trgReg}}
\index{m_trgReg@{m\_\-trgReg}!_regBlock@{\_\-reg\-Block}}
\subsubsection[m\_\-trgReg]{\setlength{\rightskip}{0pt plus 5cm}volatile unsigned int \hyperlink{struct__regBlock_o7}{\_\-reg\-Block::m\_\-trg\-Reg}}}
\label{struct__regBlock_o7}


comm i/o board self trigger register, base addr + 0x1C 

The documentation for this struct was generated from the following file:\begin{CompactItemize}
\item 
\hyperlink{reg__p_8h}{reg\_\-p.h}\end{CompactItemize}
