\hypertarget{struct__xbrd}{
\section{\_\-xbrd Struct Reference}
\label{struct__xbrd}\index{_xbrd@{\_\-xbrd}}
}
struct containing base parameters for the transition board  


{\tt \#include $<$xbrd\_\-p.h$>$}

Collaboration diagram for \_\-xbrd:\begin{figure}[H]
\begin{center}
\leavevmode
\includegraphics[width=78pt]{struct__xbrd__coll__graph}
\end{center}
\end{figure}
\subsection*{Data Fields}
\begin{CompactItemize}
\item 
unsigned int \hyperlink{struct__xbrd_o0}{m\_\-phys\-Addr}
\item 
unsigned int \hyperlink{struct__xbrd_o1}{m\_\-local\-Addr}
\item 
unsigned int \hyperlink{struct__xbrd_o2}{m\_\-detect}
\item 
unsigned int \hyperlink{struct__xbrd_o3}{m\_\-irq\-Level}
\item 
unsigned int \hyperlink{struct__xbrd_o4}{m\_\-irq\-Vec}
\item 
volatile \hyperlink{struct__xbrd__regBlock}{xbrd\_\-reg\-Block} $\ast$ \hyperlink{struct__xbrd_o5}{m\_\-base\-Addr}
\end{CompactItemize}


\subsection{Detailed Description}
struct containing base parameters for the transition board 



\subsection{Field Documentation}
\hypertarget{struct__xbrd_o5}{
\index{_xbrd@{\_\-xbrd}!m_baseAddr@{m\_\-baseAddr}}
\index{m_baseAddr@{m\_\-baseAddr}!_xbrd@{\_\-xbrd}}
\subsubsection[m\_\-baseAddr]{\setlength{\rightskip}{0pt plus 5cm}volatile \hyperlink{struct__xbrd__regBlock}{xbrd\_\-reg\-Block}$\ast$ \hyperlink{struct__xbrd_o5}{\_\-xbrd::m\_\-base\-Addr}}}
\label{struct__xbrd_o5}


pointer to transition board VME registers \hypertarget{struct__xbrd_o2}{
\index{_xbrd@{\_\-xbrd}!m_detect@{m\_\-detect}}
\index{m_detect@{m\_\-detect}!_xbrd@{\_\-xbrd}}
\subsubsection[m\_\-detect]{\setlength{\rightskip}{0pt plus 5cm}unsigned int \hyperlink{struct__xbrd_o2}{\_\-xbrd::m\_\-detect}}}
\label{struct__xbrd_o2}


Non-zero if COMM board successfully detected \hypertarget{struct__xbrd_o3}{
\index{_xbrd@{\_\-xbrd}!m_irqLevel@{m\_\-irqLevel}}
\index{m_irqLevel@{m\_\-irqLevel}!_xbrd@{\_\-xbrd}}
\subsubsection[m\_\-irqLevel]{\setlength{\rightskip}{0pt plus 5cm}unsigned int \hyperlink{struct__xbrd_o3}{\_\-xbrd::m\_\-irq\-Level}}}
\label{struct__xbrd_o3}


interrupt request level for PACKET\_\-READY \hypertarget{struct__xbrd_o4}{
\index{_xbrd@{\_\-xbrd}!m_irqVec@{m\_\-irqVec}}
\index{m_irqVec@{m\_\-irqVec}!_xbrd@{\_\-xbrd}}
\subsubsection[m\_\-irqVec]{\setlength{\rightskip}{0pt plus 5cm}unsigned int \hyperlink{struct__xbrd_o4}{\_\-xbrd::m\_\-irq\-Vec}}}
\label{struct__xbrd_o4}


interrupt vector for PACKET\_\-READY \hypertarget{struct__xbrd_o1}{
\index{_xbrd@{\_\-xbrd}!m_localAddr@{m\_\-localAddr}}
\index{m_localAddr@{m\_\-localAddr}!_xbrd@{\_\-xbrd}}
\subsubsection[m\_\-localAddr]{\setlength{\rightskip}{0pt plus 5cm}unsigned int \hyperlink{struct__xbrd_o1}{\_\-xbrd::m\_\-local\-Addr}}}
\label{struct__xbrd_o1}


local (mapped) base address of the comm board \hypertarget{struct__xbrd_o0}{
\index{_xbrd@{\_\-xbrd}!m_physAddr@{m\_\-physAddr}}
\index{m_physAddr@{m\_\-physAddr}!_xbrd@{\_\-xbrd}}
\subsubsection[m\_\-physAddr]{\setlength{\rightskip}{0pt plus 5cm}unsigned int \hyperlink{struct__xbrd_o0}{\_\-xbrd::m\_\-phys\-Addr}}}
\label{struct__xbrd_o0}


physical base address of the comm board 

The documentation for this struct was generated from the following file:\begin{CompactItemize}
\item 
\hyperlink{xbrd__p_8h}{xbrd\_\-p.h}\end{CompactItemize}
