\section{Data Structures}
Here are the data structures with brief descriptions:\begin{CompactList}
\item\contentsline{section}{\hyperlink{struct__ITC__QueueItem}{\_\-ITC\_\-Queue\-Item} (Forward reference for struct \_\-ITC\_\-Queue\-Item )}{\pageref{struct__ITC__QueueItem}}{}
\item\contentsline{section}{\hyperlink{union__LIMP__acd__off__cfg}{\_\-LIMP\_\-acd\_\-off\_\-cfg} (Union for command bitfield \hyperlink{struct__LIMP__acd__off__cfg__Bfl}{\_\-LIMP\_\-acd\_\-off\_\-cfg\_\-Bfl} )}{\pageref{union__LIMP__acd__off__cfg}}{}
\item\contentsline{section}{\hyperlink{struct__LIMP__acd__off__cfg__Bfl}{\_\-LIMP\_\-acd\_\-off\_\-cfg\_\-Bfl} (Identifies the FREE boards to power off )}{\pageref{struct__LIMP__acd__off__cfg__Bfl}}{}
\item\contentsline{section}{\hyperlink{union__LIMP__acd__on__cfg}{\_\-LIMP\_\-acd\_\-on\_\-cfg} (Union for command bitfield \hyperlink{struct__LIMP__acd__on__cfg__Bfl}{\_\-LIMP\_\-acd\_\-on\_\-cfg\_\-Bfl} )}{\pageref{union__LIMP__acd__on__cfg}}{}
\item\contentsline{section}{\hyperlink{struct__LIMP__acd__on__cfg__Bfl}{\_\-LIMP\_\-acd\_\-on\_\-cfg\_\-Bfl} (Identifies the FREE boards to power and the PDU to use )}{\pageref{struct__LIMP__acd__on__cfg__Bfl}}{}
\item\contentsline{section}{\hyperlink{struct__LIMP__EnterSAA__Pkt}{\_\-LIMP\_\-Enter\-SAA\_\-Pkt} (Command sent from the SC prior to GLAST entry into the SAA $\backslash$ APID 0xd $\backslash$ function code 3 )}{\pageref{struct__LIMP__EnterSAA__Pkt}}{}
\item\contentsline{section}{\hyperlink{union__LIMP__epu__off__cfg}{\_\-LIMP\_\-epu\_\-off\_\-cfg} (Union for command bitfield \hyperlink{struct__LIMP__epu__off__cfg__Bfl}{\_\-LIMP\_\-epu\_\-off\_\-cfg\_\-Bfl} )}{\pageref{union__LIMP__epu__off__cfg}}{}
\item\contentsline{section}{\hyperlink{struct__LIMP__epu__off__cfg__Bfl}{\_\-LIMP\_\-epu\_\-off\_\-cfg\_\-Bfl} (Identifies the EPUs to power off )}{\pageref{struct__LIMP__epu__off__cfg__Bfl}}{}
\item\contentsline{section}{\hyperlink{union__LIMP__epu__on__cfg}{\_\-LIMP\_\-epu\_\-on\_\-cfg} (Union for command bitfield \hyperlink{struct__LIMP__epu__on__cfg__Bfl}{\_\-LIMP\_\-epu\_\-on\_\-cfg\_\-Bfl} )}{\pageref{union__LIMP__epu__on__cfg}}{}
\item\contentsline{section}{\hyperlink{struct__LIMP__epu__on__cfg__Bfl}{\_\-LIMP\_\-epu\_\-on\_\-cfg\_\-Bfl} (Identifies the EPUs to power on and the PDUs to use )}{\pageref{struct__LIMP__epu__on__cfg__Bfl}}{}
\item\contentsline{section}{\hyperlink{struct__LIMP__ExitSAA__Pkt}{\_\-LIMP\_\-Exit\-SAA\_\-Pkt} (Command sent by the SC to indicate that GLAST has left the SAA $\backslash$ APID 0xd $\backslash$ function code 4 )}{\pageref{struct__LIMP__ExitSAA__Pkt}}{}
\item\contentsline{section}{\hyperlink{struct__LIMP__LoadShed__Pkt}{\_\-LIMP\_\-Load\-Shed\_\-Pkt} (Warning that SC will open main feed switch in 15 seconds $\backslash$ APID 0xd $\backslash$ function code 2 )}{\pageref{struct__LIMP__LoadShed__Pkt}}{}
\item\contentsline{section}{\hyperlink{struct__LIMP__MainFeedOn__Pkt}{\_\-LIMP\_\-Main\-Feed\-On\_\-Pkt} (Notification that the main feed switch has been closed $\backslash$ APID 0xd $\backslash$ function code 16 )}{\pageref{struct__LIMP__MainFeedOn__Pkt}}{}
\item\contentsline{section}{\hyperlink{struct__LIMP__MainFeedOn__Prm}{\_\-LIMP\_\-Main\-Feed\-On\_\-Prm} (Notification that the main feed switch has been closed $\backslash$ APID 0xd $\backslash$ function code 16 )}{\pageref{struct__LIMP__MainFeedOn__Prm}}{}
\item\contentsline{section}{\hyperlink{struct__LIMP__power__off__Pkt}{\_\-LIMP\_\-power\_\-off\_\-Pkt} (Instructs the LAT to power off some cpts $\backslash$ APID 0xd $\backslash$ function code 18 )}{\pageref{struct__LIMP__power__off__Pkt}}{}
\item\contentsline{section}{\hyperlink{struct__LIMP__power__off__Prm}{\_\-LIMP\_\-power\_\-off\_\-Prm} (Instructs the LAT to power off some cpts $\backslash$ APID 0xd $\backslash$ function code 18 )}{\pageref{struct__LIMP__power__off__Prm}}{}
\item\contentsline{section}{\hyperlink{struct__LIMP__power__on__Pkt}{\_\-LIMP\_\-power\_\-on\_\-Pkt} (Instructs the LAT to power on some cpts $\backslash$ APID 0xd $\backslash$ function code 17 )}{\pageref{struct__LIMP__power__on__Pkt}}{}
\item\contentsline{section}{\hyperlink{struct__LIMP__power__on__Prm}{\_\-LIMP\_\-power\_\-on\_\-Prm} (Instructs the LAT to power on some cpts $\backslash$ APID 0xd $\backslash$ function code 17 )}{\pageref{struct__LIMP__power__on__Prm}}{}
\item\contentsline{section}{\hyperlink{union__LIMP__siu__cfg}{\_\-LIMP\_\-siu\_\-cfg} (Union for command bitfield \hyperlink{struct__LIMP__siu__cfg__Bfl}{\_\-LIMP\_\-siu\_\-cfg\_\-Bfl} )}{\pageref{union__LIMP__siu__cfg}}{}
\item\contentsline{section}{\hyperlink{struct__LIMP__siu__cfg__Bfl}{\_\-LIMP\_\-siu\_\-cfg\_\-Bfl} (Main feed configuration )}{\pageref{struct__LIMP__siu__cfg__Bfl}}{}
\item\contentsline{section}{\hyperlink{union__LIMP__tem__off__cfg}{\_\-LIMP\_\-tem\_\-off\_\-cfg} (Union for command bitfield \hyperlink{struct__LIMP__tem__off__cfg__Bfl}{\_\-LIMP\_\-tem\_\-off\_\-cfg\_\-Bfl} )}{\pageref{union__LIMP__tem__off__cfg}}{}
\item\contentsline{section}{\hyperlink{struct__LIMP__tem__off__cfg__Bfl}{\_\-LIMP\_\-tem\_\-off\_\-cfg\_\-Bfl} (Specifies the TEMs and/or towers to power off )}{\pageref{struct__LIMP__tem__off__cfg__Bfl}}{}
\item\contentsline{section}{\hyperlink{union__LIMP__tem__on__cfg}{\_\-LIMP\_\-tem\_\-on\_\-cfg} (Union for command bitfield \hyperlink{struct__LIMP__tem__on__cfg__Bfl}{\_\-LIMP\_\-tem\_\-on\_\-cfg\_\-Bfl} )}{\pageref{union__LIMP__tem__on__cfg}}{}
\item\contentsline{section}{\hyperlink{struct__LIMP__tem__on__cfg__Bfl}{\_\-LIMP\_\-tem\_\-on\_\-cfg\_\-Bfl} (Specifies the TEMs to power on and the PDUs to use )}{\pageref{struct__LIMP__tem__on__cfg__Bfl}}{}
\item\contentsline{section}{\hyperlink{structLIMP__LHK__alert}{LIMP\_\-LHK\_\-alert} (Structure used to contain the details of an out of range alert sent from the LHK task )}{\pageref{structLIMP__LHK__alert}}{}
\end{CompactList}
