\title{The SENSEI Experiment: Status and Plans}
 
\author{Sho Uemura\\Tel Aviv University\\for the SENSEI Collaboration}
 
\date{July 20-24, 2020}
 
\documentclass[12pt]{article}
\begin{document}
\maketitle
\begin{abstract}

    SENSEI (Sub-Electron Noise Skipper Experimental Instrument) is pioneering the development of silicon CCDs with sub-electron charge resolution for low-threshold direct detection of dark matter.
    These ``skipper CCDs'' are the first detectors capable of resolving single electrons in each of millions of pixels.
    The low thresholds possible with this technology give SENSEI world-leading sensitivity to sub-GeV dark matter, which has been demonstrated in engineering runs at the surface and at a shallow underground facility.
    I present the first result from a new generation of skipper CCDs, and progress towards deployment of the 100-gram experiment at the SNOLAB deep underground facility.

\end{abstract}

\end{document}

