\hypertarget{structLCI__acdValues}{
\section{LCI\_\-acd\-Values Struct Reference}
\label{structLCI__acdValues}\index{LCI_acdValues@{LCI\_\-acdValues}}
}
The ACD register values to be used for the next calibration cycle.  


{\tt \#include $<$configure\_\-p.h$>$}

\subsection*{Data Fields}
\begin{CompactItemize}
\item 
\hypertarget{structLCI__acdValues_o0}{
unsigned short \hyperlink{structLCI__acdValues_o0}{inj}}
\label{structLCI__acdValues_o0}

\begin{CompactList}\small\item\em Charge injection magnitude. \item\end{CompactList}\item 
\hypertarget{structLCI__acdValues_o1}{
unsigned short \hyperlink{structLCI__acdValues_o1}{hld}}
\label{structLCI__acdValues_o1}

\begin{CompactList}\small\item\em High level discriminator. \item\end{CompactList}\item 
\hypertarget{structLCI__acdValues_o2}{
unsigned short \hyperlink{structLCI__acdValues_o2}{vern}}
\label{structLCI__acdValues_o2}

\begin{CompactList}\small\item\em Veto Vernier. \item\end{CompactList}\item 
\hypertarget{structLCI__acdValues_o3}{
unsigned short \hyperlink{structLCI__acdValues_o3}{veto}}
\label{structLCI__acdValues_o3}

\begin{CompactList}\small\item\em Veto threshold. \item\end{CompactList}\item 
\hypertarget{structLCI__acdValues_o4}{
unsigned short \hyperlink{structLCI__acdValues_o4}{pha}}
\label{structLCI__acdValues_o4}

\begin{CompactList}\small\item\em PHA threshold. \item\end{CompactList}\item 
\hypertarget{structLCI__acdValues_o5}{
unsigned short \hyperlink{structLCI__acdValues_o5}{bias}}
\label{structLCI__acdValues_o5}

\begin{CompactList}\small\item\em Bias DAC. \item\end{CompactList}\item 
\hypertarget{structLCI__acdValues_o6}{
unsigned short \hyperlink{structLCI__acdValues_o6}{hold}}
\label{structLCI__acdValues_o6}

\begin{CompactList}\small\item\em Hold delay. \item\end{CompactList}\item 
\hypertarget{structLCI__acdValues_o7}{
unsigned short \hyperlink{structLCI__acdValues_o7}{hitm}}
\label{structLCI__acdValues_o7}

\begin{CompactList}\small\item\em Hitmap delay. \item\end{CompactList}\item 
\hypertarget{structLCI__acdValues_o8}{
unsigned short \hyperlink{structLCI__acdValues_o8}{chnl}}
\label{structLCI__acdValues_o8}

\begin{CompactList}\small\item\em Channel to enable. \item\end{CompactList}\item 
\hypertarget{structLCI__acdValues_o9}{
unsigned short \hyperlink{structLCI__acdValues_o9}{range}}
\label{structLCI__acdValues_o9}

\begin{CompactList}\small\item\em Range bit. \item\end{CompactList}\end{CompactItemize}


\subsection{Detailed Description}
The ACD register values to be used for the next calibration cycle. 



The documentation for this struct was generated from the following file:\begin{CompactItemize}
\item 
\hyperlink{configure__p_8h}{configure\_\-p.h}\end{CompactItemize}
