\hypertarget{structLCI__calInput}{
\section{LCI\_\-cal\-Input Struct Reference}
\label{structLCI__calInput}\index{LCI_calInput@{LCI\_\-calInput}}
}
The configurable calorimeter parameters stored in a binary file.  


{\tt \#include $<$configure\_\-p.h$>$}

Collaboration diagram for LCI\_\-cal\-Input:\begin{figure}[H]
\begin{center}
\leavevmode
\includegraphics[width=56pt]{structLCI__calInput__coll__graph}
\end{center}
\end{figure}
\subsection*{Data Fields}
\begin{CompactItemize}
\item 
\hypertarget{structLCI__calInput_o0}{
unsigned \hyperlink{structLCI__calInput_o0}{first\-Rng}}
\label{structLCI__calInput_o0}

\begin{CompactList}\small\item\em First range value and use bits. \item\end{CompactList}\item 
\hypertarget{structLCI__calInput_o1}{
unsigned \hyperlink{structLCI__calInput_o1}{gain\-Le}}
\label{structLCI__calInput_o1}

\begin{CompactList}\small\item\em Low energy gain. \item\end{CompactList}\item 
\hypertarget{structLCI__calInput_o2}{
unsigned \hyperlink{structLCI__calInput_o2}{gain\-He}}
\label{structLCI__calInput_o2}

\begin{CompactList}\small\item\em High energy gain. \item\end{CompactList}\item 
\hypertarget{structLCI__calInput_o3}{
unsigned \hyperlink{structLCI__calInput_o3}{rng\-Enab\-Le}}
\label{structLCI__calInput_o3}

\begin{CompactList}\small\item\em Low energy range enable bit. \item\end{CompactList}\item 
\hypertarget{structLCI__calInput_o4}{
unsigned \hyperlink{structLCI__calInput_o4}{rng\-Enab\-He}}
\label{structLCI__calInput_o4}

\begin{CompactList}\small\item\em High energy range enable bit. \item\end{CompactList}\item 
\hypertarget{structLCI__calInput_o5}{
unsigned \hyperlink{structLCI__calInput_o5}{trg\-Enab\-Le}}
\label{structLCI__calInput_o5}

\begin{CompactList}\small\item\em Low energy trigger enable bit. \item\end{CompactList}\item 
\hypertarget{structLCI__calInput_o6}{
unsigned \hyperlink{structLCI__calInput_o6}{trg\-Enab\-He}}
\label{structLCI__calInput_o6}

\begin{CompactList}\small\item\em High energy trigger enable bit. \item\end{CompactList}\item 
\hypertarget{structLCI__calInput_o7}{
unsigned \hyperlink{structLCI__calInput_o7}{cal\-Enab\-Le}}
\label{structLCI__calInput_o7}

\begin{CompactList}\small\item\em Low energy calibration enable bit. \item\end{CompactList}\item 
\hypertarget{structLCI__calInput_o8}{
unsigned \hyperlink{structLCI__calInput_o8}{cal\-Enab\-He}}
\label{structLCI__calInput_o8}

\begin{CompactList}\small\item\em High energy calibration enable bit. \item\end{CompactList}\item 
\hypertarget{structLCI__calInput_o9}{
unsigned \hyperlink{structLCI__calInput_o9}{cal\-Gain}}
\label{structLCI__calInput_o9}

\begin{CompactList}\small\item\em Calibration gain bit. \item\end{CompactList}\item 
\hypertarget{structLCI__calInput_o10}{
\hyperlink{structLCI__cnfItem}{LCI\_\-cnf\-Item} \hyperlink{structLCI__calInput_o10}{inj}}
\label{structLCI__calInput_o10}

\begin{CompactList}\small\item\em Injection DAC. \item\end{CompactList}\item 
\hypertarget{structLCI__calInput_o11}{
\hyperlink{structLCI__cnfItem}{LCI\_\-cnf\-Item} \hyperlink{structLCI__calInput_o11}{uld}}
\label{structLCI__calInput_o11}

\begin{CompactList}\small\item\em Range Upper Level Discriminator threshold. \item\end{CompactList}\item 
\hypertarget{structLCI__calInput_o12}{
\hyperlink{structLCI__cnfItem}{LCI\_\-cnf\-Item} \hyperlink{structLCI__calInput_o12}{acc}}
\label{structLCI__calInput_o12}

\begin{CompactList}\small\item\em Trigger Accept threshold. \item\end{CompactList}\item 
\hypertarget{structLCI__calInput_o13}{
\hyperlink{structLCI__cnfItem}{LCI\_\-cnf\-Item} \hyperlink{structLCI__calInput_o13}{le}}
\label{structLCI__calInput_o13}

\begin{CompactList}\small\item\em Low Energy Trigger threshold. \item\end{CompactList}\item 
\hypertarget{structLCI__calInput_o14}{
\hyperlink{structLCI__cnfItem}{LCI\_\-cnf\-Item} \hyperlink{structLCI__calInput_o14}{he}}
\label{structLCI__calInput_o14}

\begin{CompactList}\small\item\em High Energy Trigger threshold. \item\end{CompactList}\item 
\hypertarget{structLCI__calInput_o15}{
\hyperlink{structLCI__cnfItem}{LCI\_\-cnf\-Item} \hyperlink{structLCI__calInput_o15}{col}}
\label{structLCI__calInput_o15}

\begin{CompactList}\small\item\em Columns to enable. \item\end{CompactList}\item 
\hypertarget{structLCI__calInput_o16}{
\hyperlink{structLCI__cnfItem}{LCI\_\-cnf\-Item} \hyperlink{structLCI__calInput_o16}{tack}}
\label{structLCI__calInput_o16}

\begin{CompactList}\small\item\em TACK Delay. \item\end{CompactList}\end{CompactItemize}


\subsection{Detailed Description}
The configurable calorimeter parameters stored in a binary file. 

\begin{Desc}
\item[Warning:]This structure is written to and read from the filesystem so do not add elements that are are for internal use only\end{Desc}




The documentation for this struct was generated from the following file:\begin{CompactItemize}
\item 
\hyperlink{configure__p_8h}{configure\_\-p.h}\end{CompactItemize}
