\hypertarget{structLCI__calValues}{
\section{LCI\_\-cal\-Values Struct Reference}
\label{structLCI__calValues}\index{LCI_calValues@{LCI\_\-calValues}}
}
The CAL register values to be used for the next calibration cycle.  


{\tt \#include $<$configure\_\-p.h$>$}

\subsection*{Data Fields}
\begin{CompactItemize}
\item 
\hypertarget{structLCI__calValues_o0}{
unsigned short \hyperlink{structLCI__calValues_o0}{inj}}
\label{structLCI__calValues_o0}

\begin{CompactList}\small\item\em Size of the injection. \item\end{CompactList}\item 
\hypertarget{structLCI__calValues_o1}{
unsigned short \hyperlink{structLCI__calValues_o1}{uld}}
\label{structLCI__calValues_o1}

\begin{CompactList}\small\item\em Upper level discriminator threshold. \item\end{CompactList}\item 
\hypertarget{structLCI__calValues_o2}{
unsigned short \hyperlink{structLCI__calValues_o2}{acc}}
\label{structLCI__calValues_o2}

\begin{CompactList}\small\item\em Accept threshold. \item\end{CompactList}\item 
\hypertarget{structLCI__calValues_o3}{
unsigned short \hyperlink{structLCI__calValues_o3}{le}}
\label{structLCI__calValues_o3}

\begin{CompactList}\small\item\em Low Energy trigger threshold. \item\end{CompactList}\item 
\hypertarget{structLCI__calValues_o4}{
unsigned short \hyperlink{structLCI__calValues_o4}{he}}
\label{structLCI__calValues_o4}

\begin{CompactList}\small\item\em High Energy trigger threshold. \item\end{CompactList}\item 
\hypertarget{structLCI__calValues_o5}{
unsigned short \hyperlink{structLCI__calValues_o5}{col}}
\label{structLCI__calValues_o5}

\begin{CompactList}\small\item\em Column ID to enable. \item\end{CompactList}\item 
\hypertarget{structLCI__calValues_o6}{
unsigned short \hyperlink{structLCI__calValues_o6}{tack}}
\label{structLCI__calValues_o6}

\begin{CompactList}\small\item\em Trigger sequence TACK. \item\end{CompactList}\item 
\hypertarget{structLCI__calValues_o7}{
unsigned short \hyperlink{structLCI__calValues_o7}{frst}}
\label{structLCI__calValues_o7}

\begin{CompactList}\small\item\em Use first range settings. \item\end{CompactList}\item 
\hypertarget{structLCI__calValues_o8}{
unsigned short \hyperlink{structLCI__calValues_o8}{gain\-Le}}
\label{structLCI__calValues_o8}

\begin{CompactList}\small\item\em Low energy gain. \item\end{CompactList}\item 
\hypertarget{structLCI__calValues_o9}{
unsigned short \hyperlink{structLCI__calValues_o9}{gain\-He}}
\label{structLCI__calValues_o9}

\begin{CompactList}\small\item\em High energy gain. \item\end{CompactList}\item 
\hypertarget{structLCI__calValues_o10}{
unsigned short \hyperlink{structLCI__calValues_o10}{rng\-Enab\-Le}}
\label{structLCI__calValues_o10}

\begin{CompactList}\small\item\em Low energy range enable bit. \item\end{CompactList}\item 
\hypertarget{structLCI__calValues_o11}{
unsigned short \hyperlink{structLCI__calValues_o11}{rng\-Enab\-He}}
\label{structLCI__calValues_o11}

\begin{CompactList}\small\item\em High energy range enable bit. \item\end{CompactList}\item 
\hypertarget{structLCI__calValues_o12}{
unsigned short \hyperlink{structLCI__calValues_o12}{trg\-Enab\-Le}}
\label{structLCI__calValues_o12}

\begin{CompactList}\small\item\em Low energy trigger enable bit. \item\end{CompactList}\item 
\hypertarget{structLCI__calValues_o13}{
unsigned short \hyperlink{structLCI__calValues_o13}{trg\-Enab\-He}}
\label{structLCI__calValues_o13}

\begin{CompactList}\small\item\em High energy trigger enable bit. \item\end{CompactList}\item 
\hypertarget{structLCI__calValues_o14}{
unsigned short \hyperlink{structLCI__calValues_o14}{cal\-Enab\-Le}}
\label{structLCI__calValues_o14}

\begin{CompactList}\small\item\em Low energy calibration enable bit. \item\end{CompactList}\item 
\hypertarget{structLCI__calValues_o15}{
unsigned short \hyperlink{structLCI__calValues_o15}{cal\-Enab\-He}}
\label{structLCI__calValues_o15}

\begin{CompactList}\small\item\em High energy calibration enable bit. \item\end{CompactList}\item 
\hypertarget{structLCI__calValues_o16}{
unsigned short \hyperlink{structLCI__calValues_o16}{cal\-Gain}}
\label{structLCI__calValues_o16}

\begin{CompactList}\small\item\em Calibration gain bit. \item\end{CompactList}\end{CompactItemize}


\subsection{Detailed Description}
The CAL register values to be used for the next calibration cycle. 



The documentation for this struct was generated from the following file:\begin{CompactItemize}
\item 
\hyperlink{configure__p_8h}{configure\_\-p.h}\end{CompactItemize}
