\hypertarget{struct__LayerCntsStatus}{
\section{\_\-Layer\-Cnts\-Status Struct Reference}
\label{struct__LayerCntsStatus}\index{_LayerCntsStatus@{\_\-LayerCntsStatus}}
}
Captures the result of the layer counts assessment.  


\subsection*{Data Fields}
\begin{CompactItemize}
\item 
unsigned int \hyperlink{struct__LayerCntsStatus_o0}{twr\_\-list}
\item 
unsigned short int \hyperlink{struct__LayerCntsStatus_o1}{ncmaps}
\item 
unsigned short int \hyperlink{struct__LayerCntsStatus_o2}{ncnts}
\item 
unsigned short int \hyperlink{struct__LayerCntsStatus_o3}{nstops}
\item 
unsigned int \hyperlink{struct__LayerCntsStatus_o4}{cmaps\_\-or}
\item 
unsigned int \hyperlink{struct__LayerCntsStatus_o5}{cnts\_\-width}
\item 
unsigned int \hyperlink{struct__LayerCntsStatus_o6}{cmaps} \mbox{[}16 $\ast$2\mbox{]}
\item 
unsigned char \hyperlink{struct__LayerCntsStatus_o7}{cnts} \mbox{[}16 $\ast$36 $\ast$2\mbox{]}
\end{CompactItemize}


\subsection{Detailed Description}
Captures the result of the layer counts assessment. 



\subsection{Field Documentation}
\hypertarget{struct__LayerCntsStatus_o6}{
\index{_LayerCntsStatus@{\_\-Layer\-Cnts\-Status}!cmaps@{cmaps}}
\index{cmaps@{cmaps}!_LayerCntsStatus@{\_\-Layer\-Cnts\-Status}}
\subsubsection[cmaps]{\setlength{\rightskip}{0pt plus 5cm}unsigned int \hyperlink{struct__LayerCntsStatus_o6}{\_\-Layer\-Cnts\-Status::cmaps}\mbox{[}16 $\ast$2\mbox{]}}}
\label{struct__LayerCntsStatus_o6}


Bit masks of which x y layers have cluster count information \hypertarget{struct__LayerCntsStatus_o4}{
\index{_LayerCntsStatus@{\_\-Layer\-Cnts\-Status}!cmaps_or@{cmaps\_\-or}}
\index{cmaps_or@{cmaps\_\-or}!_LayerCntsStatus@{\_\-Layer\-Cnts\-Status}}
\subsubsection[cmaps\_\-or]{\setlength{\rightskip}{0pt plus 5cm}unsigned int \hyperlink{struct__LayerCntsStatus_o4}{\_\-Layer\-Cnts\-Status::cmaps\_\-or}}}
\label{struct__LayerCntsStatus_o4}


The OR of all the count maps \hypertarget{struct__LayerCntsStatus_o7}{
\index{_LayerCntsStatus@{\_\-Layer\-Cnts\-Status}!cnts@{cnts}}
\index{cnts@{cnts}!_LayerCntsStatus@{\_\-Layer\-Cnts\-Status}}
\subsubsection[cnts]{\setlength{\rightskip}{0pt plus 5cm}unsigned char \hyperlink{struct__LayerCntsStatus_o7}{\_\-Layer\-Cnts\-Status::cnts}\mbox{[}16 $\ast$36 $\ast$2\mbox{]}}}
\label{struct__LayerCntsStatus_o7}


The counts for each layer that need it \hypertarget{struct__LayerCntsStatus_o5}{
\index{_LayerCntsStatus@{\_\-Layer\-Cnts\-Status}!cnts_width@{cnts\_\-width}}
\index{cnts_width@{cnts\_\-width}!_LayerCntsStatus@{\_\-Layer\-Cnts\-Status}}
\subsubsection[cnts\_\-width]{\setlength{\rightskip}{0pt plus 5cm}unsigned int \hyperlink{struct__LayerCntsStatus_o5}{\_\-Layer\-Cnts\-Status::cnts\_\-width}}}
\label{struct__LayerCntsStatus_o5}


Number of bits to hold the maximum layer counts field \hypertarget{struct__LayerCntsStatus_o1}{
\index{_LayerCntsStatus@{\_\-Layer\-Cnts\-Status}!ncmaps@{ncmaps}}
\index{ncmaps@{ncmaps}!_LayerCntsStatus@{\_\-Layer\-Cnts\-Status}}
\subsubsection[ncmaps]{\setlength{\rightskip}{0pt plus 5cm}unsigned short int \hyperlink{struct__LayerCntsStatus_o1}{\_\-Layer\-Cnts\-Status::ncmaps}}}
\label{struct__LayerCntsStatus_o1}


The number of cmaps \hypertarget{struct__LayerCntsStatus_o2}{
\index{_LayerCntsStatus@{\_\-Layer\-Cnts\-Status}!ncnts@{ncnts}}
\index{ncnts@{ncnts}!_LayerCntsStatus@{\_\-Layer\-Cnts\-Status}}
\subsubsection[ncnts]{\setlength{\rightskip}{0pt plus 5cm}unsigned short int \hyperlink{struct__LayerCntsStatus_o2}{\_\-Layer\-Cnts\-Status::ncnts}}}
\label{struct__LayerCntsStatus_o2}


The number cnts layers \hypertarget{struct__LayerCntsStatus_o3}{
\index{_LayerCntsStatus@{\_\-Layer\-Cnts\-Status}!nstops@{nstops}}
\index{nstops@{nstops}!_LayerCntsStatus@{\_\-Layer\-Cnts\-Status}}
\subsubsection[nstops]{\setlength{\rightskip}{0pt plus 5cm}unsigned short int \hyperlink{struct__LayerCntsStatus_o3}{\_\-Layer\-Cnts\-Status::nstops}}}
\label{struct__LayerCntsStatus_o3}


The number of strip addresses that need a stop bit. This is used to determine the cheapest encoding scheme \hypertarget{struct__LayerCntsStatus_o0}{
\index{_LayerCntsStatus@{\_\-Layer\-Cnts\-Status}!twr_list@{twr\_\-list}}
\index{twr_list@{twr\_\-list}!_LayerCntsStatus@{\_\-Layer\-Cnts\-Status}}
\subsubsection[twr\_\-list]{\setlength{\rightskip}{0pt plus 5cm}unsigned int \hyperlink{struct__LayerCntsStatus_o0}{\_\-Layer\-Cnts\-Status::twr\_\-list}}}
\label{struct__LayerCntsStatus_o0}


The list of towers class 2 and 3 towers that have a cmaps. The lowest set bit is a stop bit 

The documentation for this struct was generated from the following file:\begin{CompactItemize}
\item 
\hyperlink{CDF__tkr__std_8c}{CDF\_\-tkr\_\-std.c}\end{CompactItemize}
