\hypertarget{structLSEC__acdCompress}{
\section{LSEC\_\-acd\-Compress Struct Reference}
\label{structLSEC__acdCompress}\index{LSEC_acdCompress@{LSEC\_\-acdCompress}}
}
Private structure holding the compression information for the ACD.  


{\tt \#include $<$compact\_\-p.h$>$}

Collaboration diagram for LSEC\_\-acd\-Compress:\begin{figure}[H]
\begin{center}
\leavevmode
\includegraphics[width=123pt]{structLSEC__acdCompress__coll__graph}
\end{center}
\end{figure}
\subsection*{Data Fields}
\begin{CompactItemize}
\item 
\hyperlink{structLSEC__raw__}{LSEC\_\-raw} $\ast$ \hyperlink{structLSEC__acdCompress_o0}{raw}
\item 
\hyperlink{structLSEC__compression__}{LSEC\_\-compression} $\ast$ \hyperlink{structLSEC__acdCompress_o1}{cables}
\item 
\hyperlink{structLSEC__compression__}{LSEC\_\-compression} $\ast$ \hyperlink{structLSEC__acdCompress_o2}{chns}
\item 
\hyperlink{structLSEC__compression__}{LSEC\_\-compression} $\ast$ \hyperlink{structLSEC__acdCompress_o3}{phas}
\item 
\hyperlink{structLSEC__compression__}{LSEC\_\-compression} $\ast$ \hyperlink{structLSEC__acdCompress_o4}{pvahs}
\end{CompactItemize}


\subsection{Detailed Description}
Private structure holding the compression information for the ACD. 



\subsection{Field Documentation}
\hypertarget{structLSEC__acdCompress_o1}{
\index{LSEC_acdCompress@{LSEC\_\-acd\-Compress}!cables@{cables}}
\index{cables@{cables}!LSEC_acdCompress@{LSEC\_\-acd\-Compress}}
\subsubsection[cables]{\setlength{\rightskip}{0pt plus 5cm}\hyperlink{structLSEC__compression__}{LSEC\_\-compression}$\ast$ \hyperlink{structLSEC__acdCompress_o1}{LSEC\_\-acd\-Compress::cables}}}
\label{structLSEC__acdCompress_o1}


The electronics cable number (0-11) \hypertarget{structLSEC__acdCompress_o2}{
\index{LSEC_acdCompress@{LSEC\_\-acd\-Compress}!chns@{chns}}
\index{chns@{chns}!LSEC_acdCompress@{LSEC\_\-acd\-Compress}}
\subsubsection[chns]{\setlength{\rightskip}{0pt plus 5cm}\hyperlink{structLSEC__compression__}{LSEC\_\-compression}$\ast$ \hyperlink{structLSEC__acdCompress_o2}{LSEC\_\-acd\-Compress::chns}}}
\label{structLSEC__acdCompress_o2}


The channel number within a board (0-17) \hypertarget{structLSEC__acdCompress_o3}{
\index{LSEC_acdCompress@{LSEC\_\-acd\-Compress}!phas@{phas}}
\index{phas@{phas}!LSEC_acdCompress@{LSEC\_\-acd\-Compress}}
\subsubsection[phas]{\setlength{\rightskip}{0pt plus 5cm}\hyperlink{structLSEC__compression__}{LSEC\_\-compression}$\ast$ \hyperlink{structLSEC__acdCompress_o3}{LSEC\_\-acd\-Compress::phas}}}
\label{structLSEC__acdCompress_o3}


The PHA value, i.e. the ADC range plus the ADC value \hypertarget{structLSEC__acdCompress_o4}{
\index{LSEC_acdCompress@{LSEC\_\-acd\-Compress}!pvahs@{pvahs}}
\index{pvahs@{pvahs}!LSEC_acdCompress@{LSEC\_\-acd\-Compress}}
\subsubsection[pvahs]{\setlength{\rightskip}{0pt plus 5cm}\hyperlink{structLSEC__compression__}{LSEC\_\-compression}$\ast$ \hyperlink{structLSEC__acdCompress_o4}{LSEC\_\-acd\-Compress::pvahs}}}
\label{structLSEC__acdCompress_o4}


Combined state of the PHA parity error, PHA value valid flag, accept flag and hit flag \hypertarget{structLSEC__acdCompress_o0}{
\index{LSEC_acdCompress@{LSEC\_\-acd\-Compress}!raw@{raw}}
\index{raw@{raw}!LSEC_acdCompress@{LSEC\_\-acd\-Compress}}
\subsubsection[raw]{\setlength{\rightskip}{0pt plus 5cm}\hyperlink{structLSEC__raw__}{LSEC\_\-raw}$\ast$ \hyperlink{structLSEC__acdCompress_o0}{LSEC\_\-acd\-Compress::raw}}}
\label{structLSEC__acdCompress_o0}


nphas and nchns for each event in a cycle - uncompressed 

The documentation for this struct was generated from the following file:\begin{CompactItemize}
\item 
\hyperlink{compact__p_8h}{compact\_\-p.h}\end{CompactItemize}
