\hypertarget{structLSEC__acdCompress}{
\section{LSEC\_\-acdCompress Struct Reference}
\label{structLSEC__acdCompress}\index{LSEC_acdCompress@{LSEC\_\-acdCompress}}
}
Private structure holding the compression information for the ACD.  


{\tt \#include $<$compact\_\-p.h$>$}

\subsection*{Public Attributes}
\begin{CompactItemize}
\item 
\hypertarget{structLSEC__acdCompress_cb57093728d310ed3ecf2627a05c4176}{
\hyperlink{structLSEC__raw__}{LSEC\_\-raw} $\ast$ \hyperlink{structLSEC__acdCompress_cb57093728d310ed3ecf2627a05c4176}{raw}}
\label{structLSEC__acdCompress_cb57093728d310ed3ecf2627a05c4176}

\begin{CompactList}\small\item\em nphas and nchns for each event in a cycle\begin{itemize}
\item uncompressed \end{itemize}
\item\end{CompactList}\item 
\hypertarget{structLSEC__acdCompress_8ec0221e33893646a5d0ed6e4e9a1a26}{
\hyperlink{structLSEC__compression__}{LSEC\_\-compression} $\ast$ \hyperlink{structLSEC__acdCompress_8ec0221e33893646a5d0ed6e4e9a1a26}{cables}}
\label{structLSEC__acdCompress_8ec0221e33893646a5d0ed6e4e9a1a26}

\begin{CompactList}\small\item\em The electronics cable number (0-11). \item\end{CompactList}\item 
\hypertarget{structLSEC__acdCompress_27d6249d33dbeef5af5c7e1306232816}{
\hyperlink{structLSEC__compression__}{LSEC\_\-compression} $\ast$ \hyperlink{structLSEC__acdCompress_27d6249d33dbeef5af5c7e1306232816}{chns}}
\label{structLSEC__acdCompress_27d6249d33dbeef5af5c7e1306232816}

\begin{CompactList}\small\item\em The channel number within a board (0-17). \item\end{CompactList}\item 
\hyperlink{structLSEC__compression__}{LSEC\_\-compression} $\ast$ \hyperlink{structLSEC__acdCompress_22582f92b9b76be7c5590bf6f902f50a}{phas}
\begin{CompactList}\small\item\em The PHA value, i.e. \item\end{CompactList}\item 
\hypertarget{structLSEC__acdCompress_13d81a5b4d56d26fe52ff6814379a970}{
\hyperlink{structLSEC__compression__}{LSEC\_\-compression} $\ast$ \hyperlink{structLSEC__acdCompress_13d81a5b4d56d26fe52ff6814379a970}{pvahs}}
\label{structLSEC__acdCompress_13d81a5b4d56d26fe52ff6814379a970}

\begin{CompactList}\small\item\em Combined state of the PHA parity error, PHA value valid flag, accept flag and hit flag. \item\end{CompactList}\end{CompactItemize}


\subsection{Detailed Description}
Private structure holding the compression information for the ACD. 

\subsection{Member Data Documentation}
\hypertarget{structLSEC__acdCompress_22582f92b9b76be7c5590bf6f902f50a}{
\index{LSEC_acdCompress@{LSEC\_\-acdCompress}!phas@{phas}}
\index{phas@{phas}!LSEC_acdCompress@{LSEC\_\-acdCompress}}
\subsubsection{\setlength{\rightskip}{0pt plus 5cm}{\bf LSEC\_\-compression}$\ast$ {\bf LSEC\_\-acdCompress::phas}}}
\label{structLSEC__acdCompress_22582f92b9b76be7c5590bf6f902f50a}


The PHA value, i.e. 

the ADC range plus the ADC value 

The documentation for this struct was generated from the following file:\begin{CompactItemize}
\item 
\hyperlink{compact__p_8h}{compact\_\-p.h}\end{CompactItemize}
