\section{Data Structures}
Here are the data structures with brief descriptions:\begin{CompactList}
\item\contentsline{section}{\hyperlink{struct__ITC__QueueItem}{\_\-ITC\_\-Queue\-Item} (Forward reference for struct \_\-ITC\_\-Queue\-Item )}{\pageref{struct__ITC__QueueItem}}{}
\item\contentsline{section}{\hyperlink{struct__LTC__DiagLTC__Tlm}{\_\-LTC\_\-Diag\-LTC\_\-Tlm} (LAT Thermal Control diagnostic telemetry $\backslash$ APID 0x2bc )}{\pageref{struct__LTC__DiagLTC__Tlm}}{}
\item\contentsline{section}{\hyperlink{struct__LTC__HtrOnOffCtl__Pkt}{\_\-LTC\_\-Htr\-On\-Off\-Ctl\_\-Pkt} (Set heater to always on, or off or automatic control. $\backslash$ APID 0x645 $\backslash$ function code 5 )}{\pageref{struct__LTC__HtrOnOffCtl__Pkt}}{}
\item\contentsline{section}{\hyperlink{struct__LTC__HtrOnOffCtl__Prm}{\_\-LTC\_\-Htr\-On\-Off\-Ctl\_\-Prm} (Set heater to always on, or off or automatic control. $\backslash$ APID 0x645 $\backslash$ function code 5 )}{\pageref{struct__LTC__HtrOnOffCtl__Prm}}{}
\item\contentsline{section}{\hyperlink{union__LTC__ResRitSnsrSel}{\_\-LTC\_\-Res\-Rit\-Snsr\-Sel} (Union for telemetry bitfield \hyperlink{struct__LTC__ResRitSnsrSel__Bfl}{\_\-LTC\_\-Res\-Rit\-Snsr\-Sel\_\-Bfl} )}{\pageref{union__LTC__ResRitSnsrSel}}{}
\item\contentsline{section}{\hyperlink{struct__LTC__ResRitSnsrSel__Bfl}{\_\-LTC\_\-Res\-Rit\-Snsr\-Sel\_\-Bfl} (Selected RSVR and RIT sensors )}{\pageref{struct__LTC__ResRitSnsrSel__Bfl}}{}
\item\contentsline{section}{\hyperlink{union__LTC__ResRitStatus}{\_\-LTC\_\-Res\-Rit\-Status} (Union for telemetry bitfield \hyperlink{struct__LTC__ResRitStatus__Bfl}{\_\-LTC\_\-Res\-Rit\-Status\_\-Bfl} )}{\pageref{union__LTC__ResRitStatus}}{}
\item\contentsline{section}{\hyperlink{struct__LTC__ResRitStatus__Bfl}{\_\-LTC\_\-Res\-Rit\-Status\_\-Bfl} (Heat pipe RIT and reservoir sensors status )}{\pageref{struct__LTC__ResRitStatus__Bfl}}{}
\item\contentsline{section}{\hyperlink{struct__LTC__ReStart__Pkt}{\_\-LTC\_\-Re\-Start\_\-Pkt} (Restart and initialize Thermal Control $\backslash$ APID 0x645 $\backslash$ function code 1 )}{\pageref{struct__LTC__ReStart__Pkt}}{}
\item\contentsline{section}{\hyperlink{struct__LTC__ReStart__Prm}{\_\-LTC\_\-Re\-Start\_\-Prm} (Restart and initialize Thermal Control $\backslash$ APID 0x645 $\backslash$ function code 1 )}{\pageref{struct__LTC__ReStart__Prm}}{}
\item\contentsline{section}{\hyperlink{struct__LTC__SetMode__Pkt}{\_\-LTC\_\-Set\-Mode\_\-Pkt} (Set thermal control mode to active or passive. $\backslash$ APID 0x645 $\backslash$ function code 4 )}{\pageref{struct__LTC__SetMode__Pkt}}{}
\item\contentsline{section}{\hyperlink{struct__LTC__SetMode__Prm}{\_\-LTC\_\-Set\-Mode\_\-Prm} (Set thermal control mode to active or passive. $\backslash$ APID 0x645 $\backslash$ function code 4 )}{\pageref{struct__LTC__SetMode__Prm}}{}
\item\contentsline{section}{\hyperlink{struct__LTC__SetParam__Pkt}{\_\-LTC\_\-Set\-Param\_\-Pkt} (Set control parameters to new values. $\backslash$ APID 0x645 $\backslash$ function code 6 )}{\pageref{struct__LTC__SetParam__Pkt}}{}
\item\contentsline{section}{\hyperlink{struct__LTC__SetParam__Prm}{\_\-LTC\_\-Set\-Param\_\-Prm} (Set control parameters to new values. $\backslash$ APID 0x645 $\backslash$ function code 6 )}{\pageref{struct__LTC__SetParam__Prm}}{}
\item\contentsline{section}{\hyperlink{struct__LTC__SetTlmFreq__Pkt}{\_\-LTC\_\-Set\-Tlm\-Freq\_\-Pkt} (Set LTC telemetry frequency, 0 is off. $\backslash$ APID 0x645 $\backslash$ function code 7 )}{\pageref{struct__LTC__SetTlmFreq__Pkt}}{}
\item\contentsline{section}{\hyperlink{struct__LTC__SetTlmFreq__Prm}{\_\-LTC\_\-Set\-Tlm\-Freq\_\-Prm} (Set LTC telemetry frequency, 0 is off. $\backslash$ APID 0x645 $\backslash$ function code 7 )}{\pageref{struct__LTC__SetTlmFreq__Prm}}{}
\item\contentsline{section}{\hyperlink{struct__LTC__Start__Pkt}{\_\-LTC\_\-Start\_\-Pkt} (Start control $\backslash$ APID 0x645 $\backslash$ function code 2 )}{\pageref{struct__LTC__Start__Pkt}}{}
\item\contentsline{section}{\hyperlink{struct__LTC__Start__Prm}{\_\-LTC\_\-Start\_\-Prm} (Start control $\backslash$ APID 0x645 $\backslash$ function code 2 )}{\pageref{struct__LTC__Start__Prm}}{}
\item\contentsline{section}{\hyperlink{struct__LTC__Stop__Pkt}{\_\-LTC\_\-Stop\_\-Pkt} (Terminate Thermal Control processing $\backslash$ APID 0x645 $\backslash$ function code 3 )}{\pageref{struct__LTC__Stop__Pkt}}{}
\end{CompactList}
