\hypertarget{trigger_8c}{
\section{trigger.c File Reference}
\label{trigger_8c}\index{trigger.c@{trigger.c}}
}
Functions that trigger the LAT from the command line.  


{\tt \#include \char`\"{}DAB/reg.h\char`\"{}}\par
{\tt \#include \char`\"{}DAB/sgem.h\char`\"{}}\par


Include dependency graph for trigger.c:\begin{figure}[H]
\begin{center}
\leavevmode
\includegraphics[width=94pt]{trigger_8c__incl}
\end{center}
\end{figure}
\subsection*{Functions}
\begin{CompactItemize}
\item 
void \hyperlink{trigger_8c_a0}{trigger} (LIOXs slh, unsigned dest, unsigned n)
\begin{CompactList}\small\item\em Solicit a trigger from the GEM. \item\end{CompactList}\item 
void \hyperlink{trigger_8c_a1}{trigger\-Cnt} (LIOXs slh, unsigned dest, unsigned period, unsigned $\ast$n)
\begin{CompactList}\small\item\em Solicit a trigger from the GEM. \item\end{CompactList}\end{CompactItemize}


\subsection{Detailed Description}
Functions that trigger the LAT from the command line. 

\begin{Desc}
\item[Author:]James Swain -- \href{mailto:jswain@slac.stanford.edu}{\tt jswain@slac.stanford.edu} \end{Desc}


\subsection{Function Documentation}
\hypertarget{trigger_8c_a0}{
\index{trigger.c@{trigger.c}!trigger@{trigger}}
\index{trigger@{trigger}!trigger.c@{trigger.c}}
\subsubsection[trigger]{\setlength{\rightskip}{0pt plus 5cm}void trigger (LIOXs {\em slh}, unsigned {\em dest}, unsigned {\em n})}}
\label{trigger_8c_a0}


Solicit a trigger from the GEM. 

\begin{Desc}
\item[Parameters:]
\begin{description}
\item[{\em slh}]Synchronous LIOX handle \item[{\em dest}]Destination LCB address \item[{\em n}]Number of triggers to send \end{description}
\end{Desc}
\hypertarget{trigger_8c_a1}{
\index{trigger.c@{trigger.c}!triggerCnt@{triggerCnt}}
\index{triggerCnt@{triggerCnt}!trigger.c@{trigger.c}}
\subsubsection[triggerCnt]{\setlength{\rightskip}{0pt plus 5cm}void trigger\-Cnt (LIOXs {\em slh}, unsigned {\em dest}, unsigned {\em period}, unsigned $\ast$ {\em n})}}
\label{trigger_8c_a1}


Solicit a trigger from the GEM. 

\begin{Desc}
\item[Parameters:]
\begin{description}
\item[{\em slh}]Synchronous LIOX handle \item[{\em dest}]Destination LCB address \item[{\em n}]Pointer to counter for number of triggers sent \item[{\em period}]Period of the trigger \end{description}
\end{Desc}
