\hypertarget{dir_712def31b73c498ccc8f66a33233224f}{
\section{/afs/slac.stanford.edu/g/glast/flight/PHY/source/EDS/V2-10-1/EDS/ Directory Reference}
\label{dir_712def31b73c498ccc8f66a33233224f}\index{/afs/slac.stanford.edu/g/glast/flight/PHY/source/EDS/V2-10-1/EDS/ Directory Reference@{/afs/slac.stanford.edu/g/glast/flight/PHY/source/EDS/V2-10-1/EDS/ Directory Reference}}
}
\subsection*{Files}
\begin{CompactItemize}
\item 
file \hyperlink{ACD__rec_8h}{ACD\_\-rec.h}
\begin{CompactList}\small\item\em Defines the structure containing the unpacked the ACD record This differs from \hyperlink{EDR__acd_8h}{EDR\_\-acd.h} in that the order left in the order of ACD, not the GEM. \item\end{CompactList}

\item 
file \hyperlink{ACD__unpack_8h}{ACD\_\-unpack.h}
\begin{CompactList}\small\item\em Defines the interface to the ACD LAT unpacking routine. This is a more primitive unpacker than EDR\_\-acdUnpack meant to be used when a more barebones data structure will suffice. \item\end{CompactList}

\item 
file \hyperlink{EBF__cal_8h}{EBF\_\-cal.h}
\begin{CompactList}\small\item\em Describes the CAL data format from the event builder. \item\end{CompactList}

\item 
file \hyperlink{EBF__calEnergy_8h}{EBF\_\-calEnergy.h}
\begin{CompactList}\small\item\em Interface to sum the total energy in the CAL. \item\end{CompactList}

\item 
file \hyperlink{EBF__cid_8h}{EBF\_\-cid.h}
\begin{CompactList}\small\item\em Maps out the contributor IDs as defined by the Event Builder. \item\end{CompactList}

\item 
file \hyperlink{EBF__ctb_8h}{EBF\_\-ctb.h}
\begin{CompactList}\small\item\em Describes the attributes and data structures relating to individual contributors. \item\end{CompactList}

\item 
file \hyperlink{EBF__dir_8h}{EBF\_\-dir.h}
\begin{CompactList}\small\item\em EBF dir services, Interface. \item\end{CompactList}

\item 
file \hyperlink{EBF__ebw_8h}{EBF\_\-ebw.h}
\begin{CompactList}\small\item\em Layouts out the fields of the Event Builder Word. \item\end{CompactList}

\item 
file \hyperlink{EBF__edw_8h}{EBF\_\-edw.h}
\begin{CompactList}\small\item\em Layouts out the fields of the LCB Event (or more properly) Packet Descriptor Word packet. \item\end{CompactList}

\item 
file \hyperlink{EBF__err_8h}{EBF\_\-err.h}
\begin{CompactList}\small\item\em Maps out the TEM error contribution. \item\end{CompactList}

\item 
file \hyperlink{EBF__esw_8h}{EBF\_\-esw.h}
\begin{CompactList}\small\item\em Describes the Event Summary Word put on each contributor by The Event Builder Module. \item\end{CompactList}

\item 
file \hyperlink{EBF__evt_8h}{EBF\_\-evt.h}
\begin{CompactList}\small\item\em Defines the attributes and data structures relating to an EBF event. \item\end{CompactList}

\item 
file \hyperlink{EBF__gemLocate_8h}{EBF\_\-gemLocate.h}
\begin{CompactList}\small\item\em Locates GEM within the Event Builder Format. \item\end{CompactList}

\item 
file \hyperlink{EBF__match_8h}{EBF\_\-match.h}
\begin{CompactList}\small\item\em Interface to the EBW and ESW contributor header word matching. \item\end{CompactList}

\item 
file \hyperlink{EBF__pkt_8h}{EBF\_\-pkt.h}
\begin{CompactList}\small\item\em Defines the attributes and data structures relating to an EBF packet. \item\end{CompactList}

\item 
file \hyperlink{EBF__siv_8h}{EBF\_\-siv.h}
\begin{CompactList}\small\item\em Interface to the packet's State Information Vector. \item\end{CompactList}

\item 
file \hyperlink{EBF__tem_8h}{EBF\_\-tem.h}
\begin{CompactList}\small\item\em Describes the TEM data format from the event builder. \item\end{CompactList}

\item 
file \hyperlink{EBF__tkr_8h}{EBF\_\-tkr.h}
\begin{CompactList}\small\item\em Describes the TKR data format from the event builder. \item\end{CompactList}

\item 
file \hyperlink{ECR__acd_8h}{ECR\_\-acd.h}
\begin{CompactList}\small\item\em Interface to the ACD calibration constants utilities. \item\end{CompactList}

\item 
file \hyperlink{ECR__cal_8h}{ECR\_\-cal.h}
\begin{CompactList}\small\item\em Interface to the CAL calibration constants utilities. \item\end{CompactList}

\item 
file \hyperlink{EDA__acd_8h}{EDA\_\-acd.h}
\begin{CompactList}\small\item\em Defines basic constants about the ACD. \item\end{CompactList}

\item 
file \hyperlink{EDA__cal_8h}{EDA\_\-cal.h}
\begin{CompactList}\small\item\em Defines the event and data attributes (constants) for the CAL. \item\end{CompactList}

\item 
file \hyperlink{EDA__tkr_8h}{EDA\_\-tkr.h}
\begin{CompactList}\small\item\em Defines the event and data attributes (constants) for the TKR. \item\end{CompactList}

\item 
file \hyperlink{EDR__acd_8h}{EDR\_\-acd.h}
\begin{CompactList}\small\item\em Defines the structure containing the unpacked the ACD record. \item\end{CompactList}

\item 
file \hyperlink{EDR__acdUnpack_8h}{EDR\_\-acdUnpack.h}
\begin{CompactList}\small\item\em Defines the interface to the ACD LAT unpacking routine. \item\end{CompactList}

\item 
file \hyperlink{EDR__cal_8h}{EDR\_\-cal.h}
\begin{CompactList}\small\item\em Defines the structure containing the unpacked the calorimeter record. \item\end{CompactList}

\item 
file \hyperlink{EDR__calUnpack_8h}{EDR\_\-calUnpack.h}
\begin{CompactList}\small\item\em Defines the interface to the CAL LAT unpacking routine. \item\end{CompactList}

\item 
file \hyperlink{EDR__err_8h}{EDR\_\-err.h}
\begin{CompactList}\small\item\em Defines the structure containing the unpacked error records. \item\end{CompactList}

\item 
file \hyperlink{EDR__errUnpack_8h}{EDR\_\-errUnpack.h}
\begin{CompactList}\small\item\em Defines the interface to the ERR LAT unpacking routines. \item\end{CompactList}

\item 
file \hyperlink{EDR__tkr_8h}{EDR\_\-tkr.h}
\begin{CompactList}\small\item\em Defines the structure containing the unpacked the tracker record for all towers. \item\end{CompactList}

\item 
file \hyperlink{EDR__tkrUnpack_8h}{EDR\_\-tkrUnpack.h}
\begin{CompactList}\small\item\em Defines the interface to the TKR LAT unpacking routine. \item\end{CompactList}

\item 
file \hyperlink{EDS__cfg_8h}{EDS\_\-cfg.h}
\begin{CompactList}\small\item\em This structure defines the information needed to resolve a configuration to its original CDM file. \item\end{CompactList}

\item 
file \hyperlink{EDS__endianness_8h}{EDS\_\-endianness.h}
\begin{CompactList}\small\item\em Provides definitions of the ENDIANNESS of the target machine. The symbols {\em ENDIANNESS\_\-IS\_\-LITTLE\/} and {\em ENDIANNESS\_\-IS\_\-BIG\/} should be used in preprocessing directives to determine the endianness of the machine, while the symbol {\em ENDIANNESS\/} can be more easily used in 'C' code. \item\end{CompactList}

\item 
file \hyperlink{EDS__fw_8h}{EDS\_\-fw.h}
\begin{CompactList}\small\item\em Event Delivery Services, framework, interface. \item\end{CompactList}

\item 
file \hyperlink{EDS__fwServices_8h}{EDS\_\-fwServices.h}
\begin{CompactList}\small\item\em Defines the handler related services and parameters that are needed to register a handler. \item\end{CompactList}

\item 
file \hyperlink{EDS__rsd_8h}{EDS\_\-rsd.h}
\begin{CompactList}\small\item\em Result Summary Data Structures. \item\end{CompactList}

\item 
file \hyperlink{LCBV_8h}{LCBV.h}
\begin{CompactList}\small\item\em LCB Virtual Device, interface. \item\end{CompactList}

\end{CompactItemize}
