\section{Class List}
Here are the classes, structs, unions and interfaces with brief descriptions:\begin{CompactList}
\item\contentsline{section}{\hyperlink{struct__ACD__cableStatus}{\_\-ACD\_\-cableStatus} (Summary cable bit status masks )}{\pageref{struct__ACD__cableStatus}}{}
\item\contentsline{section}{\hyperlink{union__ACD__chn}{\_\-ACD\_\-chn} (Maps out the information for one channel, union of bit field with unsigned int )}{\pageref{union__ACD__chn}}{}
\item\contentsline{section}{\hyperlink{struct__ACD__chn__af}{\_\-ACD\_\-chn\_\-af} (Maps out the information for one ADC channel as an alternative bit field representation, where the end bit is paired with the tile address to form the extended tile address and where all the fields of the PHA vector (ADC range, ADC value and PHA parity error fields are presented as a single PHA vector field )}{\pageref{struct__ACD__chn__af}}{}
\item\contentsline{section}{\hyperlink{struct__ACD__chn__bf}{\_\-ACD\_\-chn\_\-bf} (Maps out the information for one ADC channel as the most primitve bit fields possible )}{\pageref{struct__ACD__chn__bf}}{}
\item\contentsline{section}{\hyperlink{struct__ACD__chn__cf}{\_\-ACD\_\-chn\_\-cf} (Maps out the information for one channel, as alternative bit field representation favoring consolidating all the state information as a single field and combining the ADC range and ADC value field as a single PHA field )}{\pageref{struct__ACD__chn__cf}}{}
\item\contentsline{section}{\hyperlink{struct__ACD__rec}{\_\-ACD\_\-rec} (Holds the unpacked ACD information )}{\pageref{struct__ACD__rec}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__cal}{\_\-EBF\_\-cal} (Lays out the format of the CAL data block from the event builder )}{\pageref{struct__EBF__cal}}{}
\item\contentsline{section}{\hyperlink{union__EBF__calLogData}{\_\-EBF\_\-calLogData} (Maps out the 32-bit value of a CAL log data field both in bit fields and as an unsigned 32-bit integer )}{\pageref{union__EBF__calLogData}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__calLogData__bf}{\_\-EBF\_\-calLogData\_\-bf} (Maps out the 32-bit value of a CAL log data field as bit fields )}{\pageref{struct__EBF__calLogData__bf}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__calLogData__cf}{\_\-EBF\_\-calLogData\_\-cf} (Maps out the 32-bit value of a CAL log data field as bit fields. This mapping keeps the RNG and ADC value contigious )}{\pageref{struct__EBF__calLogData__cf}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__ctb}{\_\-EBF\_\-ctb} (Template of a contributor )}{\pageref{struct__EBF__ctb}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__ctbHdr}{\_\-EBF\_\-ctbHdr} (Lays out the standard 2 header words of every contributor )}{\pageref{struct__EBF__ctbHdr}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__dir}{\_\-EBF\_\-dir} (A data structure describing all contributors data within an event )}{\pageref{struct__EBF__dir}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__dirAuxDsc}{\_\-EBF\_\-dirAuxDsc} (A data structure describing a TEMs auxillary blocks, {\em i.e\/}. the diagnostic and error blocks )}{\pageref{struct__EBF__dirAuxDsc}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__dirCtbDsc}{\_\-EBF\_\-dirCtbDsc} (A data structure describing a contributors data )}{\pageref{struct__EBF__dirCtbDsc}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__dirCtbRestart}{\_\-EBF\_\-dirCtbRestart} (Contributor restart context )}{\pageref{struct__EBF__dirCtbRestart}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__dirExpected}{\_\-EBF\_\-dirExpected} (Captures, by value, the expected values of many of the fields in the contributor header words used when checking an event for integrity )}{\pageref{struct__EBF__dirExpected}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__dirPktDsc}{\_\-EBF\_\-dirPktDsc} (Describes one packet from the sequence of packets that comprises the event )}{\pageref{struct__EBF__dirPktDsc}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__dirRedux}{\_\-EBF\_\-dirRedux} (Encapsulates information gleaned from the event's EDW and each contributor's EBWand ESW )}{\pageref{struct__EBF__dirRedux}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__dirTruncated}{\_\-EBF\_\-dirTruncated} (Collections information about truncated packets/events. This is used to reassemble the contributor )}{\pageref{struct__EBF__dirTruncated}}{}
\item\contentsline{section}{\hyperlink{union__EBF__ebw}{\_\-EBF\_\-ebw} (Defines the LATP cell header and EBM word as a union between an unsigned int and the bit field structure )}{\pageref{union__EBF__ebw}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__ebw__bf}{\_\-EBF\_\-ebw\_\-bf} (Layout of a LATP cell + EBM word )}{\pageref{struct__EBF__ebw__bf}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__ebw__us}{\_\-EBF\_\-ebw\_\-us} (Layout of a LATP cell + EBM word as unsigned short ints )}{\pageref{struct__EBF__ebw__us}}{}
\item\contentsline{section}{\hyperlink{union__EBF__edw}{\_\-EBF\_\-edw} (Union of the 32-bit integer representation and the bit-field representation of the event descriptor word )}{\pageref{union__EBF__edw}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__edw__bf}{\_\-EBF\_\-edw\_\-bf} (Map of LCB event descriptor word with broken down status fields )}{\pageref{struct__EBF__edw__bf}}{}
\item\contentsline{section}{\hyperlink{union__EBF__errGCCC}{\_\-EBF\_\-errGCCC} (The TEM CAL Common Cable error parameter as a union between its bit field representation and an uninterpretted 16-bit unsigned integer )}{\pageref{union__EBF__errGCCC}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__errGCCC__bf}{\_\-EBF\_\-errGCCC\_\-bf} (The GCCC cable error as bit fields )}{\pageref{struct__EBF__errGCCC__bf}}{}
\item\contentsline{section}{\hyperlink{union__EBF__errGTRC}{\_\-EBF\_\-errGTRC} (The TEM TKR Common Cable error summary word as a union between its bit field representation and an uninterpretted 16-bit unsigned integer )}{\pageref{union__EBF__errGTRC}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__errGTRC__bf}{\_\-EBF\_\-errGTRC\_\-bf} (The GTRC cable error as bit fields )}{\pageref{struct__EBF__errGTRC__bf}}{}
\item\contentsline{section}{\hyperlink{union__EBF__errGTRC__Phase}{\_\-EBF\_\-errGTRC\_\-Phase} (The TEM TKR Common Cable error for the GTRC phasing error as a union between its bit field representation and an uninterpretted 16-bit unsigned integer )}{\pageref{union__EBF__errGTRC__Phase}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__errGTRC__Phase__bf}{\_\-EBF\_\-errGTRC\_\-Phase\_\-bf} (The GTRC cable GTRC phasing error parameter as bit fields )}{\pageref{struct__EBF__errGTRC__Phase__bf}}{}
\item\contentsline{section}{\hyperlink{union__EBF__errTemPhase}{\_\-EBF\_\-errTemPhase} (The TEM common Cable phase error message as a union between its bit field representation and an uninterpretted 16-bit unsigned integer )}{\pageref{union__EBF__errTemPhase}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__errTemPhase__bf}{\_\-EBF\_\-errTemPhase\_\-bf} (The structure of a common cable controller phasing error message )}{\pageref{struct__EBF__errTemPhase__bf}}{}
\item\contentsline{section}{\hyperlink{union__EBF__errTemSummary}{\_\-EBF\_\-errTemSummary} (The TEM error summary word as a union between its bit field representation and an uninterpretted 16-bit unsigned integer )}{\pageref{union__EBF__errTemSummary}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__errTemSummary__bf}{\_\-EBF\_\-errTemSummary\_\-bf} (The error summary word as bit fields )}{\pageref{struct__EBF__errTemSummary__bf}}{}
\item\contentsline{section}{\hyperlink{union__EBF__errTemTimeout}{\_\-EBF\_\-errTemTimeout} (The TEM TKR Common Cable Timeout error word as a union between its bit field representation and an uninterpretted 16-bit unsigned integer )}{\pageref{union__EBF__errTemTimeout}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__errTemTimeout__bf}{\_\-EBF\_\-errTemTimeout\_\-bf} (The structure of a common cable controller timeout error message )}{\pageref{struct__EBF__errTemTimeout__bf}}{}
\item\contentsline{section}{\hyperlink{union__EBF__esw}{\_\-EBF\_\-esw} (Defines the contributor's event summary word as a union between an unsigned int and the bit field structure )}{\pageref{union__EBF__esw}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__esw__bf}{\_\-EBF\_\-esw\_\-bf} (Defines the contributor's event summary word as a bit field structure )}{\pageref{struct__EBF__esw__bf}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__evt}{\_\-EBF\_\-evt} (Template of an event as it appears in the LCB ring buffer )}{\pageref{struct__EBF__evt}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__match__LpwAssumptionChecks}{\_\-EBF\_\-match\_\-LpwAssumptionChecks} (This is a dummy structure used to check optimization assumptions )}{\pageref{struct__EBF__match__LpwAssumptionChecks}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__matchDb}{\_\-EBF\_\-matchDb} (The database defining the expected values to be used when matching the EBW and ESW )}{\pageref{struct__EBF__matchDb}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__pkt}{\_\-EBF\_\-pkt} (Template of an packet as it appears in the LCB ring buffer )}{\pageref{struct__EBF__pkt}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__pktHdr}{\_\-EBF\_\-pktHdr} (Defines the packet header area. This is the are reserve by the LCB right before the packet is dropped into the ring buffer )}{\pageref{struct__EBF__pktHdr}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__pktRestartCell}{\_\-EBF\_\-pktRestartCell} (Defines the restart cell )}{\pageref{struct__EBF__pktRestartCell}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__pktRestartHdr}{\_\-EBF\_\-pktRestartHdr} (Defines the restart packet header )}{\pageref{struct__EBF__pktRestartHdr}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__tem}{\_\-EBF\_\-tem} (Lays out the format of the TEM data block from the event builder )}{\pageref{struct__EBF__tem}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__temDiag}{\_\-EBF\_\-temDiag} (Lays out the TEM diagnostic block )}{\pageref{struct__EBF__temDiag}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__temDiagCal}{\_\-EBF\_\-temDiagCal} (The CAL portion of the TEM diagnostic block )}{\pageref{struct__EBF__temDiagCal}}{}
\item\contentsline{section}{\hyperlink{union__EBF__temDiagGCCC}{\_\-EBF\_\-temDiagGCCC} (Union of all the different representations of the one diagnostic GCCC layer word )}{\pageref{union__EBF__temDiagGCCC}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__temDiagGCCC__np}{\_\-EBF\_\-temDiagGCCC\_\-np} (Layout of one a GCCC as negative/positive pair of GCRCs )}{\pageref{struct__EBF__temDiagGCCC__np}}{}
\item\contentsline{section}{\hyperlink{union__EBF__temDiagGCRC}{\_\-EBF\_\-temDiagGCRC} (Union of the bit-field representation of one TEM GCRC diagnostic word with an uninterpretted 16-bit representation )}{\pageref{union__EBF__temDiagGCRC}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__temDiagGCRC__bf}{\_\-EBF\_\-temDiagGCRC\_\-bf} (Layout of the GCRC diagnostic block as bit fields )}{\pageref{struct__EBF__temDiagGCRC__bf}}{}
\item\contentsline{section}{\hyperlink{union__EBF__temDiagGTCC}{\_\-EBF\_\-temDiagGTCC} (Union of the 16-bit and bit-field representations of the TEM GTCC diagnostic contribution )}{\pageref{union__EBF__temDiagGTCC}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__temDiagGTCC__bf}{\_\-EBF\_\-temDiagGTCC\_\-bf} (Layout of the GCRC diagnostic block as bit fields )}{\pageref{struct__EBF__temDiagGTCC__bf}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__temDiagGTCCpair}{\_\-EBF\_\-temDiagGTCCpair} (Layouts of the 32-bit word representing the odd and even halves of either and X/Y hi/lo set of GTCCs )}{\pageref{struct__EBF__temDiagGTCCpair}}{}
\item\contentsline{section}{\hyperlink{union__EBF__temDiagTkr}{\_\-EBF\_\-temDiagTkr} (Union of the various representations of the TKR GTCCs )}{\pageref{union__EBF__temDiagTkr}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__tkr}{\_\-EBF\_\-tkr} (Lays out the format of the TKR data block from the event builder )}{\pageref{struct__EBF__tkr}}{}
\item\contentsline{section}{\hyperlink{struct__ECR__acd}{\_\-ECR\_\-acd} (The combination of the ACD pedestals and gains )}{\pageref{struct__ECR__acd}}{}
\item\contentsline{section}{\hyperlink{union__ECR__acdPedestals}{\_\-ECR\_\-acdPedestals} (The ACD pedestals referenced by either a flat index or by cable )}{\pageref{union__ECR__acdPedestals}}{}
\item\contentsline{section}{\hyperlink{struct__ECR__acdPedestalsBoard}{\_\-ECR\_\-acdPedestalsBoard} (Defines the pedestals for one range of one FREE board )}{\pageref{struct__ECR__acdPedestalsBoard}}{}
\item\contentsline{section}{\hyperlink{union__ECR__acdPedestalsRange}{\_\-ECR\_\-acdPedestalsRange} (The ACD pedestals referenced by either a flat index or by board )}{\pageref{union__ECR__acdPedestalsRange}}{}
\item\contentsline{section}{\hyperlink{struct__ECR__cal}{\_\-ECR\_\-cal} (The calibration constants for CAL )}{\pageref{struct__ECR__cal}}{}
\item\contentsline{section}{\hyperlink{union__ECR__calLayer}{\_\-ECR\_\-calLayer} (The calibration constants for one range of one layer )}{\pageref{union__ECR__calLayer}}{}
\item\contentsline{section}{\hyperlink{struct__ECR__calLog}{\_\-ECR\_\-calLog} (The calibration constants for one range of one log )}{\pageref{struct__ECR__calLog}}{}
\item\contentsline{section}{\hyperlink{union__ECR__calLogEnd}{\_\-ECR\_\-calLogEnd} (The calibration constants for one range of one log end )}{\pageref{union__ECR__calLogEnd}}{}
\item\contentsline{section}{\hyperlink{struct__ECR__calLogEnd__bf}{\_\-ECR\_\-calLogEnd\_\-bf} (The calibration constants for one range of one log end, bit field representation )}{\pageref{struct__ECR__calLogEnd__bf}}{}
\item\contentsline{section}{\hyperlink{union__ECR__calRange}{\_\-ECR\_\-calRange} (The calibration constants for one ranges of a one tower )}{\pageref{union__ECR__calRange}}{}
\item\contentsline{section}{\hyperlink{union__ECR__calTower}{\_\-ECR\_\-calTower} (The calibration constants for all ranges of a one tower )}{\pageref{union__ECR__calTower}}{}
\item\contentsline{section}{\hyperlink{struct__EDR__acd}{\_\-EDR\_\-acd} (Holds the unpacked ACD information )}{\pageref{struct__EDR__acd}}{}
\item\contentsline{section}{\hyperlink{struct__EDR__acdRemap}{\_\-EDR\_\-acdRemap} (Defines the information necessary to remap all ACD information laid out in electronics space to a geographical space )}{\pageref{struct__EDR__acdRemap}}{}
\item\contentsline{section}{\hyperlink{struct__EDR__acdRemapBrd}{\_\-EDR\_\-acdRemapBrd} (Structure defining the remapping the ACD data on a single board from electronics space into the standard 4 geographically oriented lists )}{\pageref{struct__EDR__acdRemapBrd}}{}
\item\contentsline{section}{\hyperlink{struct__EDR__cal}{\_\-EDR\_\-cal} (Structure containing the unpacked CAL data for all towers )}{\pageref{struct__EDR__cal}}{}
\item\contentsline{section}{\hyperlink{struct__EDR__calTower}{\_\-EDR\_\-calTower} (Structure containing the unpacked CAL data for this tower )}{\pageref{struct__EDR__calTower}}{}
\item\contentsline{section}{\hyperlink{struct__EDR__err}{\_\-EDR\_\-err} (The unpacked error records )}{\pageref{struct__EDR__err}}{}
\item\contentsline{section}{\hyperlink{struct__EDR__errCal}{\_\-EDR\_\-errCal} (The unpacked CAL error record )}{\pageref{struct__EDR__errCal}}{}
\item\contentsline{section}{\hyperlink{union__EDR__errCalStatus}{\_\-EDR\_\-errCalStatus} (The status word as union between an uninterpretted 32-bit integer an its bit field representation )}{\pageref{union__EDR__errCalStatus}}{}
\item\contentsline{section}{\hyperlink{struct__EDR__errCalStatus__bf}{\_\-EDR\_\-errCalStatus\_\-bf} (The status word as bit fields )}{\pageref{struct__EDR__errCalStatus__bf}}{}
\item\contentsline{section}{\hyperlink{union__EDR__errGCCCStatus}{\_\-EDR\_\-errGCCCStatus} (The status word as union between an uninterpretted 32-bit integer an its bit field representation )}{\pageref{union__EDR__errGCCCStatus}}{}
\item\contentsline{section}{\hyperlink{struct__EDR__errGCCCStatus__bf}{\_\-EDR\_\-errGCCCStatus\_\-bf} (The status word as bit fields )}{\pageref{struct__EDR__errGCCCStatus__bf}}{}
\item\contentsline{section}{\hyperlink{struct__EDR__errGTCC}{\_\-EDR\_\-errGTCC} (The unpacked GTCC information )}{\pageref{struct__EDR__errGTCC}}{}
\item\contentsline{section}{\hyperlink{union__EDR__errGTCCStatus}{\_\-EDR\_\-errGTCCStatus} (The status word as union between an uninterpretted 32-bit integer an its bit field representation )}{\pageref{union__EDR__errGTCCStatus}}{}
\item\contentsline{section}{\hyperlink{struct__EDR__errGTCCStatus__bf}{\_\-EDR\_\-errGTCCStatus\_\-bf} (The status word as bit fields )}{\pageref{struct__EDR__errGTCCStatus__bf}}{}
\item\contentsline{section}{\hyperlink{struct__EDR__errGTRC}{\_\-EDR\_\-errGTRC} (The unpacked GTRC information )}{\pageref{struct__EDR__errGTRC}}{}
\item\contentsline{section}{\hyperlink{union__EDR__errStatus}{\_\-EDR\_\-errStatus} (Union of the different representations of the error unpacking status )}{\pageref{union__EDR__errStatus}}{}
\item\contentsline{section}{\hyperlink{struct__EDR__errStatusConditions__bf}{\_\-EDR\_\-errStatusConditions\_\-bf} (The conditions part of the status word )}{\pageref{struct__EDR__errStatusConditions__bf}}{}
\item\contentsline{section}{\hyperlink{struct__EDR__errTem}{\_\-EDR\_\-errTem} (The unpacked error record for one TEM )}{\pageref{struct__EDR__errTem}}{}
\item\contentsline{section}{\hyperlink{struct__EDR__errTemPhase}{\_\-EDR\_\-errTemPhase} (The unpacked data for the TEM PHASE error component )}{\pageref{struct__EDR__errTemPhase}}{}
\item\contentsline{section}{\hyperlink{union__EDR__errTemPhaseStatus}{\_\-EDR\_\-errTemPhaseStatus} (The status word as union between an uninterpretted 32-bit integer an its bit field representation )}{\pageref{union__EDR__errTemPhaseStatus}}{}
\item\contentsline{section}{\hyperlink{struct__EDR__errTemPhaseStatus__bf}{\_\-EDR\_\-errTemPhaseStatus\_\-bf} (The status word as bit fields )}{\pageref{struct__EDR__errTemPhaseStatus__bf}}{}
\item\contentsline{section}{\hyperlink{struct__EDR__errTemSummary}{\_\-EDR\_\-errTemSummary} (The unpacked TEM error summary record )}{\pageref{struct__EDR__errTemSummary}}{}
\item\contentsline{section}{\hyperlink{struct__EDR__errTemTimeout}{\_\-EDR\_\-errTemTimeout} (The unpacked data for the TEM TIMEOUT error component )}{\pageref{struct__EDR__errTemTimeout}}{}
\item\contentsline{section}{\hyperlink{union__EDR__errTemTimeoutStatus}{\_\-EDR\_\-errTemTimeoutStatus} (The status word as union between an uninterpretted 32-bit integer an its bit field representation )}{\pageref{union__EDR__errTemTimeoutStatus}}{}
\item\contentsline{section}{\hyperlink{struct__EDR__errTemTimeoutStatus__bf}{\_\-EDR\_\-errTemTimeoutStatus\_\-bf} (The status word as bit fields )}{\pageref{struct__EDR__errTemTimeoutStatus__bf}}{}
\item\contentsline{section}{\hyperlink{struct__EDR__errTkr}{\_\-EDR\_\-errTkr} (The unpacked TKR error record )}{\pageref{struct__EDR__errTkr}}{}
\item\contentsline{section}{\hyperlink{union__EDR__errTkrStatus}{\_\-EDR\_\-errTkrStatus} (The status word as union between an uninterpretted 32-bit integer an its bit field representation )}{\pageref{union__EDR__errTkrStatus}}{}
\item\contentsline{section}{\hyperlink{struct__EDR__errTkrStatus__bf}{\_\-EDR\_\-errTkrStatus\_\-bf} (The status word as bit fields )}{\pageref{struct__EDR__errTkrStatus__bf}}{}
\item\contentsline{section}{\hyperlink{struct__EDR__tkr}{\_\-EDR\_\-tkr} (Structure containing the unpacked TKR data for all towers )}{\pageref{struct__EDR__tkr}}{}
\item\contentsline{section}{\hyperlink{struct__EDR__tkrCluster}{\_\-EDR\_\-tkrCluster} (Defines a track cluster as consisting of the center of the cluster, its width and the ladder gap correction factor )}{\pageref{struct__EDR__tkrCluster}}{}
\item\contentsline{section}{\hyperlink{struct__EDR__tkrLayer}{\_\-EDR\_\-tkrLayer} (Information about the hit strips in one layer )}{\pageref{struct__EDR__tkrLayer}}{}
\item\contentsline{section}{\hyperlink{struct__EDR__tkrTower}{\_\-EDR\_\-tkrTower} (Structure containing the unpacked TKR data for this tower )}{\pageref{struct__EDR__tkrTower}}{}
\item\contentsline{section}{\hyperlink{struct__EDS__cfgInfo}{\_\-EDS\_\-cfgInfo} (This is contains information about a configuration. In general, it is filled by the EDS\_\-fwHandlerSelect callbacks and distributed by EDS\_\-fwPostNotifyRtn. Note that handlers do not need to be notified, since they are the ones implementing the selection )}{\pageref{struct__EDS__cfgInfo}}{}
\item\contentsline{section}{\hyperlink{struct__EDS__fw}{\_\-EDS\_\-fw} (The encompassing EDS frame control structure )}{\pageref{struct__EDS__fw}}{}
\item\contentsline{section}{\hyperlink{struct__EDS__fwEvt}{\_\-EDS\_\-fwEvt} (These are the reserved data blocks used in the EDS\_\-fwIxb )}{\pageref{struct__EDS__fwEvt}}{}
\item\contentsline{section}{\hyperlink{struct__EDS__fwFateNeeds}{\_\-EDS\_\-fwFateNeeds} (This keeps track of both the statically declared needs and the currently active needs )}{\pageref{struct__EDS__fwFateNeeds}}{}
\item\contentsline{section}{\hyperlink{struct__EDS__fwHandler}{\_\-EDS\_\-fwHandler} (Holds the context for one registered callback handler )}{\pageref{struct__EDS__fwHandler}}{}
\item\contentsline{section}{\hyperlink{struct__EDS__fwHandlerCfgs}{\_\-EDS\_\-fwHandlerCfgs} (Holds the current configuration for each of the installed handlers )}{\pageref{struct__EDS__fwHandlerCfgs}}{}
\item\contentsline{section}{\hyperlink{struct__EDS__fwHandlerRegisteredServices}{\_\-EDS\_\-fwHandlerRegisteredServices} (The registered services )}{\pageref{struct__EDS__fwHandlerRegisteredServices}}{}
\item\contentsline{section}{\hyperlink{struct__EDS__fwHandlerServices}{\_\-EDS\_\-fwHandlerServices} (Event handler services )}{\pageref{struct__EDS__fwHandlerServices}}{}
\item\contentsline{section}{\hyperlink{struct__EDS__fwHandlerServicesX1}{\_\-EDS\_\-fwHandlerServicesX1} (Event handler servicesX1 )}{\pageref{struct__EDS__fwHandlerServicesX1}}{}
\item\contentsline{section}{\hyperlink{struct__EDS__fwIxb}{\_\-EDS\_\-fwIxb} (Encapsulates all the derived data structures associated with an event )}{\pageref{struct__EDS__fwIxb}}{}
\item\contentsline{section}{\hyperlink{union__EDS__fwIxbBlk}{\_\-EDS\_\-fwIxbBlk} (The pointer data block )}{\pageref{union__EDS__fwIxbBlk}}{}
\item\contentsline{section}{\hyperlink{struct__EDS__fwIxbDst}{\_\-EDS\_\-fwIxbDst} (Static information about the nature of the data sinking controlled by this EDS framework )}{\pageref{struct__EDS__fwIxbDst}}{}
\item\contentsline{section}{\hyperlink{struct__EDS__fwIxbInfo}{\_\-EDS\_\-fwIxbInfo} (Derived information about the event that is can be shared between processor )}{\pageref{struct__EDS__fwIxbInfo}}{}
\item\contentsline{section}{\hyperlink{struct__EDS__fwIxbObjAddDef}{\_\-EDS\_\-fwIxbObjAddDef} (Defines an object to add to the EDS\_\-fwIxb table )}{\pageref{struct__EDS__fwIxbObjAddDef}}{}
\item\contentsline{section}{\hyperlink{struct__EDS__fwIxbObjDsc}{\_\-EDS\_\-fwIxbObjDsc} (Describes the static properties of the framework's event objects )}{\pageref{struct__EDS__fwIxbObjDsc}}{}
\item\contentsline{section}{\hyperlink{struct__EDS__fwIxbObjTbl}{\_\-EDS\_\-fwIxbObjTbl} (The table of managed objects )}{\pageref{struct__EDS__fwIxbObjTbl}}{}
\item\contentsline{section}{\hyperlink{struct__EDS__fwIxbSrc}{\_\-EDS\_\-fwIxbSrc} (Static information about the nature of the data source controlled by this EDS framework )}{\pageref{struct__EDS__fwIxbSrc}}{}
\item\contentsline{section}{\hyperlink{struct__EDS__fwLists}{\_\-EDS\_\-fwLists} (Manages both the static and dynamic lists of the framework )}{\pageref{struct__EDS__fwLists}}{}
\item\contentsline{section}{\hyperlink{struct__EDS__fwMem}{\_\-EDS\_\-fwMem} (The memory manager for the framework )}{\pageref{struct__EDS__fwMem}}{}
\item\contentsline{section}{\hyperlink{struct__EDS__fwPktFree}{\_\-EDS\_\-fwPktFree} (The LCB event free context )}{\pageref{struct__EDS__fwPktFree}}{}
\item\contentsline{section}{\hyperlink{struct__EDS__fwPostCtl}{\_\-EDS\_\-fwPostCtl} (The post context structure )}{\pageref{struct__EDS__fwPostCtl}}{}
\item\contentsline{section}{\hyperlink{struct__EDS__fwPoster}{\_\-EDS\_\-fwPoster} (The post context structure for one poster )}{\pageref{struct__EDS__fwPoster}}{}
\item\contentsline{section}{\hyperlink{struct__EDS__fwPostServices}{\_\-EDS\_\-fwPostServices} (The services as a structure )}{\pageref{struct__EDS__fwPostServices}}{}
\item\contentsline{section}{\hyperlink{struct__EDS__fwSynchCtx}{\_\-EDS\_\-fwSynchCtx} (The context needed to synchronize with the event deliver task )}{\pageref{struct__EDS__fwSynchCtx}}{}
\item\contentsline{section}{\hyperlink{struct__EDS__rsdDsc}{\_\-EDS\_\-rsdDsc} (Descriptor for the result summary data )}{\pageref{struct__EDS__rsdDsc}}{}
\item\contentsline{section}{\hyperlink{struct__EDS__rsdTbl}{\_\-EDS\_\-rsdTbl} (The result summary data table )}{\pageref{struct__EDS__rsdTbl}}{}
\item\contentsline{section}{\hyperlink{union__TKR__2strips}{\_\-TKR\_\-2strips} (Maps out the first word containing strip addresses )}{\pageref{union__TKR__2strips}}{}
\item\contentsline{section}{\hyperlink{struct__TKR__2strips__bf}{\_\-TKR\_\-2strips\_\-bf} (Maps out the first word containing strip addresses )}{\pageref{struct__TKR__2strips__bf}}{}
\item\contentsline{section}{\hyperlink{union__TKR__8strips0}{\_\-TKR\_\-8strips0} (Maps out the first word of the 3 strip address pattern words as bit fields and uninterpretted 32-bit integer )}{\pageref{union__TKR__8strips0}}{}
\item\contentsline{section}{\hyperlink{struct__TKR__8strips0__bf}{\_\-TKR\_\-8strips0\_\-bf} (Maps out the first word of the 3 strip address pattern words as bit fields )}{\pageref{struct__TKR__8strips0__bf}}{}
\item\contentsline{section}{\hyperlink{union__TKR__8strips1}{\_\-TKR\_\-8strips1} (Maps out the second word of the 3 strip address pattern words as bit fields and uninterpretted 32-bit integer )}{\pageref{union__TKR__8strips1}}{}
\item\contentsline{section}{\hyperlink{struct__TKR__8strips1__bf}{\_\-TKR\_\-8strips1\_\-bf} (Maps out the second word of the 3 strip address pattern words as bit fields )}{\pageref{struct__TKR__8strips1__bf}}{}
\item\contentsline{section}{\hyperlink{union__TKR__8strips2}{\_\-TKR\_\-8strips2} (Maps out the third word of the 3 strip address pattern words as bit fields and uninterpretted 32-bit integer )}{\pageref{union__TKR__8strips2}}{}
\item\contentsline{section}{\hyperlink{struct__TKR__8strips2__bf}{\_\-TKR\_\-8strips2\_\-bf} (Maps out the third word of the 3 strip address pattern words as bit fields )}{\pageref{struct__TKR__8strips2__bf}}{}
\item\contentsline{section}{\hyperlink{structEDR__errGCCC}{EDR\_\-errGCCC} (The error words associated with one GCCC )}{\pageref{structEDR__errGCCC}}{}
\end{CompactList}
