\section{Class List}
Here are the classes, structs, unions and interfaces with brief descriptions:\begin{CompactList}
\item\contentsline{section}{\hyperlink{union__EBF__ebw}{\_\-EBF\_\-ebw} (Defines the LATP cell header and EBM word as a union between an unsigned int and the bit field structure )}{\pageref{union__EBF__ebw}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__ebw__bf}{\_\-EBF\_\-ebw\_\-bf} (Layout of a LATP cell + EBM word )}{\pageref{struct__EBF__ebw__bf}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__ebw__us}{\_\-EBF\_\-ebw\_\-us} (Layout of a LATP cell + EBM word as unsigned short ints )}{\pageref{struct__EBF__ebw__us}}{}
\item\contentsline{section}{\hyperlink{union__EBF__edw}{\_\-EBF\_\-edw} (Union of the 32-bit integer representation and the bit-field representation of the event descriptor word )}{\pageref{union__EBF__edw}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__edw__bf}{\_\-EBF\_\-edw\_\-bf} (Map of LCB event descriptor word with broken down status fields )}{\pageref{struct__EBF__edw__bf}}{}
\item\contentsline{section}{\hyperlink{union__EBF__errGCCC}{\_\-EBF\_\-errGCCC} (The TEM CAL Common Cable error parameter as a union between its bit field representation and an uninterpretted 16-bit unsigned integer )}{\pageref{union__EBF__errGCCC}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__errGCCC__bf}{\_\-EBF\_\-errGCCC\_\-bf} (The GCCC cable error as bit fields )}{\pageref{struct__EBF__errGCCC__bf}}{}
\item\contentsline{section}{\hyperlink{union__EBF__errGTRC}{\_\-EBF\_\-errGTRC} (The TEM TKR Common Cable error summary word as a union between its bit field representation and an uninterpretted 16-bit unsigned integer )}{\pageref{union__EBF__errGTRC}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__errGTRC__bf}{\_\-EBF\_\-errGTRC\_\-bf} (The GTRC cable error as bit fields )}{\pageref{struct__EBF__errGTRC__bf}}{}
\item\contentsline{section}{\hyperlink{union__EBF__errGTRC__Phase}{\_\-EBF\_\-errGTRC\_\-Phase} (The TEM TKR Common Cable error for the GTRC phasing error as a union between its bit field representation and an uninterpretted 16-bit unsigned integer )}{\pageref{union__EBF__errGTRC__Phase}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__errGTRC__Phase__bf}{\_\-EBF\_\-errGTRC\_\-Phase\_\-bf} (The GTRC cable GTRC phasing error parameter as bit fields )}{\pageref{struct__EBF__errGTRC__Phase__bf}}{}
\item\contentsline{section}{\hyperlink{union__EBF__errTemPhase}{\_\-EBF\_\-errTemPhase} (The TEM common Cable phase error message as a union between its bit field representation and an uninterpretted 16-bit unsigned integer )}{\pageref{union__EBF__errTemPhase}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__errTemPhase__bf}{\_\-EBF\_\-errTemPhase\_\-bf} (The structure of a common cable controller phasing error message )}{\pageref{struct__EBF__errTemPhase__bf}}{}
\item\contentsline{section}{\hyperlink{union__EBF__errTemSummary}{\_\-EBF\_\-errTemSummary} (The TEM error summary word as a union between its bit field representation and an uninterpretted 16-bit unsigned integer )}{\pageref{union__EBF__errTemSummary}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__errTemSummary__bf}{\_\-EBF\_\-errTemSummary\_\-bf} (The error summary word as bit fields )}{\pageref{struct__EBF__errTemSummary__bf}}{}
\item\contentsline{section}{\hyperlink{union__EBF__errTemTimeout}{\_\-EBF\_\-errTemTimeout} (The TEM TKR Common Cable Timeout error word as a union between its bit field representation and an uninterpretted 16-bit unsigned integer )}{\pageref{union__EBF__errTemTimeout}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__errTemTimeout__bf}{\_\-EBF\_\-errTemTimeout\_\-bf} (The structure of a common cable controller timeout error message )}{\pageref{struct__EBF__errTemTimeout__bf}}{}
\item\contentsline{section}{\hyperlink{union__EBF__esw}{\_\-EBF\_\-esw} (Defines the contributor's event summary word as a union between an unsigned int and the bit field structure )}{\pageref{union__EBF__esw}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__esw__bf}{\_\-EBF\_\-esw\_\-bf} (Defines the contributor's event summary word as a bit field structure )}{\pageref{struct__EBF__esw__bf}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__mc}{\_\-EBF\_\-mc} (Defines the packet header area when it contains Monte Carlo Information )}{\pageref{struct__EBF__mc}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__tem}{\_\-EBF\_\-tem} (Lays out the format of the TEM data block from the event builder )}{\pageref{struct__EBF__tem}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__temDiag}{\_\-EBF\_\-temDiag} (Lays out the TEM diagnostic block )}{\pageref{struct__EBF__temDiag}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__temDiagCal}{\_\-EBF\_\-temDiagCal} (The CAL portion of the TEM diagnostic block )}{\pageref{struct__EBF__temDiagCal}}{}
\item\contentsline{section}{\hyperlink{union__EBF__temDiagGCCC}{\_\-EBF\_\-temDiagGCCC} (Union of all the different representations of the one diagnostic GCCC layer word )}{\pageref{union__EBF__temDiagGCCC}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__temDiagGCCC__np}{\_\-EBF\_\-temDiagGCCC\_\-np} (Layout of one a GCCC as negative/positive pair of GCRCs )}{\pageref{struct__EBF__temDiagGCCC__np}}{}
\item\contentsline{section}{\hyperlink{union__EBF__temDiagGCRC}{\_\-EBF\_\-temDiagGCRC} (Union of the bit-field representation of one TEM GCRC diagnostic word with an uninterpretted 16-bit representation )}{\pageref{union__EBF__temDiagGCRC}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__temDiagGCRC__bf}{\_\-EBF\_\-temDiagGCRC\_\-bf} (Layout of the GCRC diagnostic block as bit fields )}{\pageref{struct__EBF__temDiagGCRC__bf}}{}
\item\contentsline{section}{\hyperlink{union__EBF__temDiagGTCC}{\_\-EBF\_\-temDiagGTCC} (Union of the 16-bit and bit-field representations of the TEM GTCC diagnostic contribution )}{\pageref{union__EBF__temDiagGTCC}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__temDiagGTCC__bf}{\_\-EBF\_\-temDiagGTCC\_\-bf} (Layout of the GCRC diagnostic block as bit fields )}{\pageref{struct__EBF__temDiagGTCC__bf}}{}
\item\contentsline{section}{\hyperlink{struct__EBF__temDiagGTCCpair}{\_\-EBF\_\-temDiagGTCCpair} (Layouts of the 32-bit word representing the odd and even halves of either and X/Y hi/lo set of GTCCs )}{\pageref{struct__EBF__temDiagGTCCpair}}{}
\item\contentsline{section}{\hyperlink{union__EBF__temDiagTkr}{\_\-EBF\_\-temDiagTkr} (Union of the various representations of the TKR GTCCs )}{\pageref{union__EBF__temDiagTkr}}{}
\item\contentsline{section}{\hyperlink{struct__EDR__err}{\_\-EDR\_\-err} (The unpacked error records )}{\pageref{struct__EDR__err}}{}
\item\contentsline{section}{\hyperlink{struct__EDR__errCal}{\_\-EDR\_\-errCal} (The unpacked CAL error record )}{\pageref{struct__EDR__errCal}}{}
\item\contentsline{section}{\hyperlink{union__EDR__errCalStatus}{\_\-EDR\_\-errCalStatus} (The status word as union between an uninterpretted 32-bit integer an its bit field representation )}{\pageref{union__EDR__errCalStatus}}{}
\item\contentsline{section}{\hyperlink{struct__EDR__errCalStatus__bf}{\_\-EDR\_\-errCalStatus\_\-bf} (The status word as bit fields )}{\pageref{struct__EDR__errCalStatus__bf}}{}
\item\contentsline{section}{\hyperlink{union__EDR__errGCCCStatus}{\_\-EDR\_\-errGCCCStatus} (The status word as union between an uninterpretted 32-bit integer an its bit field representation )}{\pageref{union__EDR__errGCCCStatus}}{}
\item\contentsline{section}{\hyperlink{struct__EDR__errGCCCStatus__bf}{\_\-EDR\_\-errGCCCStatus\_\-bf} (The status word as bit fields )}{\pageref{struct__EDR__errGCCCStatus__bf}}{}
\item\contentsline{section}{\hyperlink{struct__EDR__errGTCC}{\_\-EDR\_\-errGTCC} (The unpacked GTCC information )}{\pageref{struct__EDR__errGTCC}}{}
\item\contentsline{section}{\hyperlink{union__EDR__errGTCCStatus}{\_\-EDR\_\-errGTCCStatus} (The status word as union between an uninterpretted 32-bit integer an its bit field representation )}{\pageref{union__EDR__errGTCCStatus}}{}
\item\contentsline{section}{\hyperlink{struct__EDR__errGTCCStatus__bf}{\_\-EDR\_\-errGTCCStatus\_\-bf} (The status word as bit fields )}{\pageref{struct__EDR__errGTCCStatus__bf}}{}
\item\contentsline{section}{\hyperlink{struct__EDR__errGTRC}{\_\-EDR\_\-errGTRC} (The unpacked GTRC information )}{\pageref{struct__EDR__errGTRC}}{}
\item\contentsline{section}{\hyperlink{union__EDR__errStatus}{\_\-EDR\_\-errStatus} (Union of the different representations of the error unpacking status )}{\pageref{union__EDR__errStatus}}{}
\item\contentsline{section}{\hyperlink{struct__EDR__errStatusConditions__bf}{\_\-EDR\_\-errStatusConditions\_\-bf} (The conditions part of the status word )}{\pageref{struct__EDR__errStatusConditions__bf}}{}
\item\contentsline{section}{\hyperlink{struct__EDR__errTem}{\_\-EDR\_\-errTem} (The unpacked error record for one TEM )}{\pageref{struct__EDR__errTem}}{}
\item\contentsline{section}{\hyperlink{struct__EDR__errTemPhase}{\_\-EDR\_\-errTemPhase} (The unpacked data for the TEM PHASE error component )}{\pageref{struct__EDR__errTemPhase}}{}
\item\contentsline{section}{\hyperlink{union__EDR__errTemPhaseStatus}{\_\-EDR\_\-errTemPhaseStatus} (The status word as union between an uninterpretted 32-bit integer an its bit field representation )}{\pageref{union__EDR__errTemPhaseStatus}}{}
\item\contentsline{section}{\hyperlink{struct__EDR__errTemPhaseStatus__bf}{\_\-EDR\_\-errTemPhaseStatus\_\-bf} (The status word as bit fields )}{\pageref{struct__EDR__errTemPhaseStatus__bf}}{}
\item\contentsline{section}{\hyperlink{struct__EDR__errTemSummary}{\_\-EDR\_\-errTemSummary} (The unpacked TEM error summary record )}{\pageref{struct__EDR__errTemSummary}}{}
\item\contentsline{section}{\hyperlink{struct__EDR__errTemTimeout}{\_\-EDR\_\-errTemTimeout} (The unpacked data for the TEM TIMEOUT error component )}{\pageref{struct__EDR__errTemTimeout}}{}
\item\contentsline{section}{\hyperlink{union__EDR__errTemTimeoutStatus}{\_\-EDR\_\-errTemTimeoutStatus} (The status word as union between an uninterpretted 32-bit integer an its bit field representation )}{\pageref{union__EDR__errTemTimeoutStatus}}{}
\item\contentsline{section}{\hyperlink{struct__EDR__errTemTimeoutStatus__bf}{\_\-EDR\_\-errTemTimeoutStatus\_\-bf} (The status word as bit fields )}{\pageref{struct__EDR__errTemTimeoutStatus__bf}}{}
\item\contentsline{section}{\hyperlink{struct__EDR__errTkr}{\_\-EDR\_\-errTkr} (The unpacked TKR error record )}{\pageref{struct__EDR__errTkr}}{}
\item\contentsline{section}{\hyperlink{union__EDR__errTkrStatus}{\_\-EDR\_\-errTkrStatus} (The status word as union between an uninterpretted 32-bit integer an its bit field representation )}{\pageref{union__EDR__errTkrStatus}}{}
\item\contentsline{section}{\hyperlink{struct__EDR__errTkrStatus__bf}{\_\-EDR\_\-errTkrStatus\_\-bf} (The status word as bit fields )}{\pageref{struct__EDR__errTkrStatus__bf}}{}
\item\contentsline{section}{\hyperlink{struct__EDS__cfgInfo}{\_\-EDS\_\-cfgInfo} (This is contains information about a configuration. In general, it is filled by the EDS\_\-fwHandlerSelect callbacks and distributed by EDS\_\-fwPostNotifyRtn. Note that handlers do not need to be notified, since they are the ones implementing the selection )}{\pageref{struct__EDS__cfgInfo}}{}
\item\contentsline{section}{\hyperlink{struct__EDS__fwHandlerServices}{\_\-EDS\_\-fwHandlerServices} (Event handler services )}{\pageref{struct__EDS__fwHandlerServices}}{}
\item\contentsline{section}{\hyperlink{struct__EDS__fwHandlerServicesX1}{\_\-EDS\_\-fwHandlerServicesX1} (Event handler servicesX1 )}{\pageref{struct__EDS__fwHandlerServicesX1}}{}
\item\contentsline{section}{\hyperlink{struct__EDS__fwPostServices}{\_\-EDS\_\-fwPostServices} (The services as a structure )}{\pageref{struct__EDS__fwPostServices}}{}
\item\contentsline{section}{\hyperlink{struct__EDS__rsdDsc}{\_\-EDS\_\-rsdDsc} (Descriptor for the result summary data )}{\pageref{struct__EDS__rsdDsc}}{}
\item\contentsline{section}{\hyperlink{struct__EDS__rsdTbl}{\_\-EDS\_\-rsdTbl} (The result summary data table )}{\pageref{struct__EDS__rsdTbl}}{}
\item\contentsline{section}{\hyperlink{struct__EDSD__printCtl}{\_\-EDSD\_\-printCtl} (Print control block )}{\pageref{struct__EDSD__printCtl}}{}
\item\contentsline{section}{\hyperlink{struct__EDSD__sivCtl}{\_\-EDSD\_\-sivCtl} (The control structure for the SIV demo/test )}{\pageref{struct__EDSD__sivCtl}}{}
\item\contentsline{section}{\hyperlink{struct__EDSD__size}{\_\-EDSD\_\-size} (Describes the event-by-event sizes of the contributions )}{\pageref{struct__EDSD__size}}{}
\item\contentsline{section}{\hyperlink{struct__EDSD__sizesCtl}{\_\-EDSD\_\-sizesCtl} (Control block for evaluating the sizes of various components of an event )}{\pageref{struct__EDSD__sizesCtl}}{}
\item\contentsline{section}{\hyperlink{struct__EDSD__sizesSummary}{\_\-EDSD\_\-sizesSummary} (Holds the derived sizes )}{\pageref{struct__EDSD__sizesSummary}}{}
\item\contentsline{section}{\hyperlink{struct__EDSD__sizeTem}{\_\-EDSD\_\-sizeTem} (The total size and sizes of the TEM record components )}{\pageref{struct__EDSD__sizeTem}}{}
\item\contentsline{section}{\hyperlink{struct__EDSD__tkrCtl}{\_\-EDSD\_\-tkrCtl} (The control structure for the SIV demo/test )}{\pageref{struct__EDSD__tkrCtl}}{}
\item\contentsline{section}{\hyperlink{struct__EDSD__unpackCtl}{\_\-EDSD\_\-unpackCtl} (Demonstration/test of the basic unpacking routines control block )}{\pageref{struct__EDSD__unpackCtl}}{}
\item\contentsline{section}{\hyperlink{struct__EDSD__unpackRecord}{\_\-EDSD\_\-unpackRecord} (Information about the unpacking of one object )}{\pageref{struct__EDSD__unpackRecord}}{}
\item\contentsline{section}{\hyperlink{struct__EDSD__unpackResult}{\_\-EDSD\_\-unpackResult} (Information about the unpacking of one event )}{\pageref{struct__EDSD__unpackResult}}{}
\item\contentsline{section}{\hyperlink{struct__EDSD__unpackSummary}{\_\-EDSD\_\-unpackSummary} (Summary result record )}{\pageref{struct__EDSD__unpackSummary}}{}
\item\contentsline{section}{\hyperlink{struct__TkrTowerCnts}{\_\-TkrTowerCnts} (Consolidates various global statistics about a tower )}{\pageref{struct__TkrTowerCnts}}{}
\item\contentsline{section}{\hyperlink{structEDR__errGCCC}{EDR\_\-errGCCC} (The error words associated with one GCCC )}{\pageref{structEDR__errGCCC}}{}
\end{CompactList}
