\hypertarget{struct__GammaCfgAcd}{
\section{\_\-Gamma\-Cfg\-Acd Struct Reference}
\label{struct__GammaCfgAcd}\index{_GammaCfgAcd@{\_\-GammaCfgAcd}}
}
System control structure for the evaluate ACD.  


{\tt \#include $<$GFC\_\-def.h$>$}

Collaboration diagram for \_\-Gamma\-Cfg\-Acd:\begin{figure}[H]
\begin{center}
\leavevmode
\includegraphics[width=75pt]{struct__GammaCfgAcd__coll__graph}
\end{center}
\end{figure}
\subsection*{Data Fields}
\begin{CompactItemize}
\item 
unsigned int \hyperlink{struct__GammaCfgAcd_o0}{top\-Side\-Emax}
\item 
unsigned int \hyperlink{struct__GammaCfgAcd_o1}{top\-Side\-Filter\-Emax}
\item 
unsigned int \hyperlink{struct__GammaCfgAcd_o2}{splash\-Emax}
\item 
unsigned int \hyperlink{struct__GammaCfgAcd_o3}{splash\-Count}
\item 
const \hyperlink{struct__AFC__splashMap}{AFC\_\-splash\-Map} $\ast$ \hyperlink{struct__GammaCfgAcd_o4}{splash\-Map}
\end{CompactItemize}


\subsection{Detailed Description}
System control structure for the evaluate ACD. 



\subsection{Field Documentation}
\hypertarget{struct__GammaCfgAcd_o3}{
\index{_GammaCfgAcd@{\_\-Gamma\-Cfg\-Acd}!splashCount@{splashCount}}
\index{splashCount@{splashCount}!_GammaCfgAcd@{\_\-Gamma\-Cfg\-Acd}}
\subsubsection[splashCount]{\setlength{\rightskip}{0pt plus 5cm}unsigned int \hyperlink{struct__GammaCfgAcd_o3}{\_\-Gamma\-Cfg\-Acd::splash\-Count}}}
\label{struct__GammaCfgAcd_o3}


Maximum tile count for events exceeding {\em splash\-Emax\/}. This is $>$= comparison, so if the value is 4 then events with energy greater than 40000 Mev and ACD tiles $>$=4 get rejected \hypertarget{struct__GammaCfgAcd_o2}{
\index{_GammaCfgAcd@{\_\-Gamma\-Cfg\-Acd}!splashEmax@{splashEmax}}
\index{splashEmax@{splashEmax}!_GammaCfgAcd@{\_\-Gamma\-Cfg\-Acd}}
\subsubsection[splashEmax]{\setlength{\rightskip}{0pt plus 5cm}unsigned int \hyperlink{struct__GammaCfgAcd_o2}{\_\-Gamma\-Cfg\-Acd::splash\-Emax}}}
\label{struct__GammaCfgAcd_o2}


Maximum energy to apply maximum tile count and the splash veto typical 40000 Mev \hypertarget{struct__GammaCfgAcd_o4}{
\index{_GammaCfgAcd@{\_\-Gamma\-Cfg\-Acd}!splashMap@{splashMap}}
\index{splashMap@{splashMap}!_GammaCfgAcd@{\_\-Gamma\-Cfg\-Acd}}
\subsubsection[splashMap]{\setlength{\rightskip}{0pt plus 5cm}const \hyperlink{struct__AFC__splashMap}{AFC\_\-splash\-Map}$\ast$ \hyperlink{struct__GammaCfgAcd_o4}{\_\-Gamma\-Cfg\-Acd::splash\-Map}}}
\label{struct__GammaCfgAcd_o4}


The splash map to use, this defines the near and far neighbors of each tile. \hypertarget{struct__GammaCfgAcd_o0}{
\index{_GammaCfgAcd@{\_\-Gamma\-Cfg\-Acd}!topSideEmax@{topSideEmax}}
\index{topSideEmax@{topSideEmax}!_GammaCfgAcd@{\_\-Gamma\-Cfg\-Acd}}
\subsubsection[topSideEmax]{\setlength{\rightskip}{0pt plus 5cm}unsigned int \hyperlink{struct__GammaCfgAcd_o0}{\_\-Gamma\-Cfg\-Acd::top\-Side\-Emax}}}
\label{struct__GammaCfgAcd_o0}


Maximum energy to apply top and side vetoes, Typical 10Me\-V, GFC\_\-STATUS\_\-M\_\-EO\_\-TILE \hypertarget{struct__GammaCfgAcd_o1}{
\index{_GammaCfgAcd@{\_\-Gamma\-Cfg\-Acd}!topSideFilterEmax@{topSideFilterEmax}}
\index{topSideFilterEmax@{topSideFilterEmax}!_GammaCfgAcd@{\_\-Gamma\-Cfg\-Acd}}
\subsubsection[topSideFilterEmax]{\setlength{\rightskip}{0pt plus 5cm}unsigned int \hyperlink{struct__GammaCfgAcd_o1}{\_\-Gamma\-Cfg\-Acd::top\-Side\-Filter\-Emax}}}
\label{struct__GammaCfgAcd_o1}


Maximum energy to apply top and side filter (rows 0 \& 1), typical 350 Mev 

The documentation for this struct was generated from the following file:\begin{CompactItemize}
\item 
\hyperlink{GFC__def_8h}{GFC\_\-def.h}\end{CompactItemize}
