\hypertarget{struct__GammaCfgCal}{
\section{\_\-Gamma\-Cfg\-Cal Struct Reference}
\label{struct__GammaCfgCal}\index{_GammaCfgCal@{\_\-GammaCfgCal}}
}
System control structure for the CAL cuts.  


{\tt \#include $<$GFC\_\-def.h$>$}

\subsection*{Data Fields}
\begin{CompactItemize}
\item 
int \hyperlink{struct__GammaCfgCal_o0}{epass}
\item 
int \hyperlink{struct__GammaCfgCal_o1}{eveto}
\item 
int \hyperlink{struct__GammaCfgCal_o2}{emin}
\item 
int \hyperlink{struct__GammaCfgCal_o3}{emax}
\item 
unsigned int \hyperlink{struct__GammaCfgCal_o4}{layer0Ratio\-Lo}
\item 
unsigned int \hyperlink{struct__GammaCfgCal_o5}{layer0Ratio\-Hi}
\end{CompactItemize}


\subsection{Detailed Description}
System control structure for the CAL cuts. 



\subsection{Field Documentation}
\hypertarget{struct__GammaCfgCal_o3}{
\index{_GammaCfgCal@{\_\-Gamma\-Cfg\-Cal}!emax@{emax}}
\index{emax@{emax}!_GammaCfgCal@{\_\-Gamma\-Cfg\-Cal}}
\subsubsection[emax]{\setlength{\rightskip}{0pt plus 5cm}int \hyperlink{struct__GammaCfgCal_o3}{\_\-Gamma\-Cfg\-Cal::emax}}}
\label{struct__GammaCfgCal_o3}


The limiting energy for doing the layer ratio test, typically 300Me\-V, \hypertarget{struct__GammaCfgCal_o2}{
\index{_GammaCfgCal@{\_\-Gamma\-Cfg\-Cal}!emin@{emin}}
\index{emin@{emin}!_GammaCfgCal@{\_\-Gamma\-Cfg\-Cal}}
\subsubsection[emin]{\setlength{\rightskip}{0pt plus 5cm}int \hyperlink{struct__GammaCfgCal_o2}{\_\-Gamma\-Cfg\-Cal::emin}}}
\label{struct__GammaCfgCal_o2}


The lower energy limit for doing the layer ratio test \hypertarget{struct__GammaCfgCal_o0}{
\index{_GammaCfgCal@{\_\-Gamma\-Cfg\-Cal}!epass@{epass}}
\index{epass@{epass}!_GammaCfgCal@{\_\-Gamma\-Cfg\-Cal}}
\subsubsection[epass]{\setlength{\rightskip}{0pt plus 5cm}int \hyperlink{struct__GammaCfgCal_o0}{\_\-Gamma\-Cfg\-Cal::epass}}}
\label{struct__GammaCfgCal_o0}


The hi energy pass value \hypertarget{struct__GammaCfgCal_o1}{
\index{_GammaCfgCal@{\_\-Gamma\-Cfg\-Cal}!eveto@{eveto}}
\index{eveto@{eveto}!_GammaCfgCal@{\_\-Gamma\-Cfg\-Cal}}
\subsubsection[eveto]{\setlength{\rightskip}{0pt plus 5cm}int \hyperlink{struct__GammaCfgCal_o1}{\_\-Gamma\-Cfg\-Cal::eveto}}}
\label{struct__GammaCfgCal_o1}


The lo energy veto value \hypertarget{struct__GammaCfgCal_o5}{
\index{_GammaCfgCal@{\_\-Gamma\-Cfg\-Cal}!layer0RatioHi@{layer0RatioHi}}
\index{layer0RatioHi@{layer0RatioHi}!_GammaCfgCal@{\_\-Gamma\-Cfg\-Cal}}
\subsubsection[layer0RatioHi]{\setlength{\rightskip}{0pt plus 5cm}unsigned int \hyperlink{struct__GammaCfgCal_o5}{\_\-Gamma\-Cfg\-Cal::layer0Ratio\-Hi}}}
\label{struct__GammaCfgCal_o5}


The low end layer ratio cut, typically 90\%, this is expressed in units of 1024, so 900 $\sim$= 90\% \hypertarget{struct__GammaCfgCal_o4}{
\index{_GammaCfgCal@{\_\-Gamma\-Cfg\-Cal}!layer0RatioLo@{layer0RatioLo}}
\index{layer0RatioLo@{layer0RatioLo}!_GammaCfgCal@{\_\-Gamma\-Cfg\-Cal}}
\subsubsection[layer0RatioLo]{\setlength{\rightskip}{0pt plus 5cm}unsigned int \hyperlink{struct__GammaCfgCal_o4}{\_\-Gamma\-Cfg\-Cal::layer0Ratio\-Lo}}}
\label{struct__GammaCfgCal_o4}


The low end layer ratio cut, typically 1\%, this is expressed in units of 1024, so 10 $\sim$= 1\% 

The documentation for this struct was generated from the following file:\begin{CompactItemize}
\item 
\hyperlink{GFC__def_8h}{GFC\_\-def.h}\end{CompactItemize}
