\section{Class List}
Here are the classes, structs, unions and interfaces with brief descriptions:\begin{CompactList}
\item\contentsline{section}{\hyperlink{struct__ASC}{\_\-ASC} (The control structure for an ASC process )}{\pageref{struct__ASC}}{}
\item\contentsline{section}{\hyperlink{struct__ASC__ascBdy__Gzip0}{\_\-ASC\_\-ascBdy\_\-Gzip0} (Structure of the GZIP'd compressed ASC histogram )}{\pageref{struct__ASC__ascBdy__Gzip0}}{}
\item\contentsline{section}{\hyperlink{struct__ASC__ascBdy__Raw0}{\_\-ASC\_\-ascBdy\_\-Raw0} (Structure of the uncompressed ASC histogram )}{\pageref{struct__ASC__ascBdy__Raw0}}{}
\item\contentsline{section}{\hyperlink{struct__ASC__ascCtb__Gzip0}{\_\-ASC\_\-ascCtb\_\-Gzip0} (The ASC data contribution, counters + body )}{\pageref{struct__ASC__ascCtb__Gzip0}}{}
\item\contentsline{section}{\hyperlink{struct__ASC__ascCtb__Raw0}{\_\-ASC\_\-ascCtb\_\-Raw0} (The ASC data contribution, header + body )}{\pageref{struct__ASC__ascCtb__Raw0}}{}
\item\contentsline{section}{\hyperlink{struct__ASC__cno}{\_\-ASC\_\-cno} (Accumulates the counts for the CNO vector )}{\pageref{struct__ASC__cno}}{}
\item\contentsline{section}{\hyperlink{struct__ASC__cnts}{\_\-ASC\_\-cnts} (Statistics for each of the 4 lists )}{\pageref{struct__ASC__cnts}}{}
\item\contentsline{section}{\hyperlink{struct__ASC__counters}{\_\-ASC\_\-counters} (All ACD counts )}{\pageref{struct__ASC__counters}}{}
\item\contentsline{section}{\hyperlink{struct__ASC__handlerConstructCfg}{\_\-ASC\_\-handlerConstructCfg} (Defines the configuration parameters for the Construct routine )}{\pageref{struct__ASC__handlerConstructCfg}}{}
\item\contentsline{section}{\hyperlink{struct__ASC__list}{\_\-ASC\_\-list} (The ACD vector counts for each of the 32 ACD readout channels is in a list )}{\pageref{struct__ASC__list}}{}
\item\contentsline{section}{\hyperlink{struct__ASC__patterns}{\_\-ASC\_\-patterns} (Accumulates the pattern counts for one ACD FREE board channel )}{\pageref{struct__ASC__patterns}}{}
\item\contentsline{section}{\hyperlink{struct__ASC__stats}{\_\-ASC\_\-stats} (ASC monitoring statistics )}{\pageref{struct__ASC__stats}}{}
\item\contentsline{section}{\hyperlink{struct__EMP__ASCEPU0__Tlm}{\_\-EMP\_\-ASCEPU0\_\-Tlm} (ASC stats from ACD/GEM processed on EPU0 $\backslash$ APID 0x3da )}{\pageref{struct__EMP__ASCEPU0__Tlm}}{}
\item\contentsline{section}{\hyperlink{struct__EMP__ASCEPU1__Tlm}{\_\-EMP\_\-ASCEPU1\_\-Tlm} (ASC stats from ACD/GEM processed on EPU1 $\backslash$ APID 0x3db )}{\pageref{struct__EMP__ASCEPU1__Tlm}}{}
\item\contentsline{section}{\hyperlink{struct__EMP__ASCEPU2__Tlm}{\_\-EMP\_\-ASCEPU2\_\-Tlm} (ASC stats from ACD/GEM processed on EPU2 $\backslash$ APID 0x3dc )}{\pageref{struct__EMP__ASCEPU2__Tlm}}{}
\item\contentsline{section}{\hyperlink{struct__EMP__ASCEPU3__Tlm}{\_\-EMP\_\-ASCEPU3\_\-Tlm} (ASC stats from ACD/GEM processed on EPU3 $\backslash$ APID 0x3dd )}{\pageref{struct__EMP__ASCEPU3__Tlm}}{}
\item\contentsline{section}{\hyperlink{struct__EMP__ASCSIU__Tlm}{\_\-EMP\_\-ASCSIU\_\-Tlm} (ASC stats from ACD/GEM processed on SIU $\backslash$ APID 0x3d9 )}{\pageref{struct__EMP__ASCSIU__Tlm}}{}
\item\contentsline{section}{\hyperlink{struct__EMP__hdr}{\_\-EMP\_\-hdr} (EMP standard header for event-based statistics )}{\pageref{struct__EMP__hdr}}{}
\item\contentsline{section}{\hyperlink{struct__EMP__hdrEvt}{\_\-EMP\_\-hdrEvt} (Captures the information needed to uniquely identify this event by sequence and time )}{\pageref{struct__EMP__hdrEvt}}{}
\item\contentsline{section}{\hyperlink{struct__EMP__hdrEvtSeq}{\_\-EMP\_\-hdrEvtSeq} (Hide the access to the long long to avoid alignment issues )}{\pageref{struct__EMP__hdrEvtSeq}}{}
\item\contentsline{section}{\hyperlink{struct__EMP__hdrEvtSpan}{\_\-EMP\_\-hdrEvtSpan} (The defining information about the first and last event that went into the sample )}{\pageref{struct__EMP__hdrEvtSpan}}{}
\item\contentsline{section}{\hyperlink{struct__EMP__hdrTimetone}{\_\-EMP\_\-hdrTimetone} (Defines the most general version of the timetone information )}{\pageref{struct__EMP__hdrTimetone}}{}
\item\contentsline{section}{\hyperlink{struct__EMP__hdrTimetones}{\_\-EMP\_\-hdrTimetones} (Captures the information needed to convert a GEM event clock register value into an absolute time )}{\pageref{struct__EMP__hdrTimetones}}{}
\item\contentsline{section}{\hyperlink{struct__EMP__writeCbp}{\_\-EMP\_\-writeCbp} (Binds the routine to write an ITC queue item with its context parameter )}{\pageref{struct__EMP__writeCbp}}{}
\item\contentsline{section}{\hyperlink{struct__Flush}{\_\-Flush} (Flush control structure )}{\pageref{struct__Flush}}{}
\item\contentsline{section}{\hyperlink{struct__FlushMessage}{\_\-FlushMessage} (Flush fork message structure )}{\pageref{struct__FlushMessage}}{}
\item\contentsline{section}{\hyperlink{struct__LastEvent}{\_\-LastEvent} (Information about the last event in the previous packet. This used to seed the begin information of the next packet )}{\pageref{struct__LastEvent}}{}
\item\contentsline{section}{\hyperlink{struct__LCB__header}{\_\-LCB\_\-header} (Layouts out the header for an LCB packet. The header is represented in terms of 32-bit quantities to avoid BIG/ LITTLE endian problems )}{\pageref{struct__LCB__header}}{}
\item\contentsline{section}{\hyperlink{struct__LSD__sdi}{\_\-LSD\_\-sdi} (Context structure for formatting and writing data to the SDI )}{\pageref{struct__LSD__sdi}}{}
\item\contentsline{section}{\hyperlink{struct__LSD__sdiWriteCbp}{\_\-LSD\_\-sdiWriteCbp} (Binds the routine to write an ITC queue item with its context parameter )}{\pageref{struct__LSD__sdiWriteCbp}}{}
\item\contentsline{section}{\hyperlink{struct__OutputMessage}{\_\-OutputMessage} (This is a buffer with a header large enough to hold the control information to both store this on the FPA free que and post it to an output FORK que. The body of the message is the buffer for the output datagram )}{\pageref{struct__OutputMessage}}{}
\item\contentsline{section}{\hyperlink{struct__Prescaler}{\_\-Prescaler} (Prescaler control structure )}{\pageref{struct__Prescaler}}{}
\end{CompactList}
