\hypertarget{struct__MfcCfgCal}{
\section{\_\-Mfc\-Cfg\-Cal Struct Reference}
\label{struct__MfcCfgCal}\index{_MfcCfgCal@{\_\-MfcCfgCal}}
}
System control structure for the CAL cuts.  


{\tt \#include $<$MFC\_\-def.h$>$}

\subsection*{Data Fields}
\begin{CompactItemize}
\item 
unsigned int \hyperlink{struct__MfcCfgCal_o0}{elo}
\item 
unsigned int \hyperlink{struct__MfcCfgCal_o1}{ehi}
\item 
unsigned int \hyperlink{struct__MfcCfgCal_o2}{nlayers}
\end{CompactItemize}


\subsection{Detailed Description}
System control structure for the CAL cuts. 



\subsection{Field Documentation}
\hypertarget{struct__MfcCfgCal_o1}{
\index{_MfcCfgCal@{\_\-Mfc\-Cfg\-Cal}!ehi@{ehi}}
\index{ehi@{ehi}!_MfcCfgCal@{\_\-Mfc\-Cfg\-Cal}}
\subsubsection[ehi]{\setlength{\rightskip}{0pt plus 5cm}unsigned int \hyperlink{struct__MfcCfgCal_o1}{\_\-Mfc\-Cfg\-Cal::ehi}}}
\label{struct__MfcCfgCal_o1}


The upper energy threshold, expressed in 2$\ast$LEUS, used to determine if the energy deposited is in the 1 MIP range. With a MIP in the CAL being $\sim$12 Mev, this number is typically set to $\sim$20 Mev \hypertarget{struct__MfcCfgCal_o0}{
\index{_MfcCfgCal@{\_\-Mfc\-Cfg\-Cal}!elo@{elo}}
\index{elo@{elo}!_MfcCfgCal@{\_\-Mfc\-Cfg\-Cal}}
\subsubsection[elo]{\setlength{\rightskip}{0pt plus 5cm}unsigned int \hyperlink{struct__MfcCfgCal_o0}{\_\-Mfc\-Cfg\-Cal::elo}}}
\label{struct__MfcCfgCal_o0}


The lower energy threshold, expressed in 2$\ast$LEUs, used to determine if the energy deposited is in the 1 MIP range. With a MIP in the CAL being $\sim$12 Mev, this number is typically set to $\sim$5 Mev \hypertarget{struct__MfcCfgCal_o2}{
\index{_MfcCfgCal@{\_\-Mfc\-Cfg\-Cal}!nlayers@{nlayers}}
\index{nlayers@{nlayers}!_MfcCfgCal@{\_\-Mfc\-Cfg\-Cal}}
\subsubsection[nlayers]{\setlength{\rightskip}{0pt plus 5cm}unsigned int \hyperlink{struct__MfcCfgCal_o2}{\_\-Mfc\-Cfg\-Cal::nlayers}}}
\label{struct__MfcCfgCal_o2}


The number of layers to check for minimum ionizing. The test for failure is greater than this value. Typical value is 3 

The documentation for this struct was generated from the following file:\begin{CompactItemize}
\item 
\hyperlink{MFC__def_8h}{MFC\_\-def.h}\end{CompactItemize}
