\hypertarget{struct__WCT}{
\section{\_\-WCT Struct Reference}
\label{struct__WCT}\index{_WCT@{\_\-WCT}}
}
Internal control struct for the WCT facility.  


Collaboration diagram for \_\-WCT:\begin{figure}[H]
\begin{center}
\leavevmode
\includegraphics[width=58pt]{struct__WCT__coll__graph}
\end{center}
\end{figure}
\subsection*{Data Fields}
\begin{CompactItemize}
\item 
\hyperlink{struct__LSU__factors}{LSU\_\-factors} \hyperlink{struct__WCT_o0}{p\-TOa}
\item 
\hyperlink{WCT_8h_a11}{WCT\_\-time} \hyperlink{struct__WCT_o1}{atime}
\item 
unsigned int \hyperlink{struct__WCT_o2}{ptime}
\item 
\hyperlink{struct__LSU__factors}{LSU\_\-factors} \hyperlink{struct__WCT_o3}{a\-TOp}
\item 
unsigned int \hyperlink{struct__WCT_o4}{aticks}
\item 
unsigned int \hyperlink{struct__WCT_o5}{pticks}
\end{CompactItemize}


\subsection{Detailed Description}
Internal control struct for the WCT facility. 



\subsection{Field Documentation}
\hypertarget{struct__WCT_o4}{
\index{_WCT@{\_\-WCT}!aticks@{aticks}}
\index{aticks@{aticks}!_WCT@{\_\-WCT}}
\subsubsection[aticks]{\setlength{\rightskip}{0pt plus 5cm}unsigned int \hyperlink{struct__WCT_o4}{\_\-WCT::aticks}}}
\label{struct__WCT_o4}


An elapsed number of absolute ticks \hypertarget{struct__WCT_o1}{
\index{_WCT@{\_\-WCT}!atime@{atime}}
\index{atime@{atime}!_WCT@{\_\-WCT}}
\subsubsection[atime]{\setlength{\rightskip}{0pt plus 5cm}\hyperlink{WCT_8h_a11}{WCT\_\-time} \hyperlink{struct__WCT_o1}{\_\-WCT::atime}}}
\label{struct__WCT_o1}


The last known absolute time \hypertarget{struct__WCT_o3}{
\index{_WCT@{\_\-WCT}!aTOp@{aTOp}}
\index{aTOp@{aTOp}!_WCT@{\_\-WCT}}
\subsubsection[aTOp]{\setlength{\rightskip}{0pt plus 5cm}\hyperlink{struct__LSU__factors}{LSU\_\-factors} \hyperlink{struct__WCT_o3}{\_\-WCT::a\-TOp}}}
\label{struct__WCT_o3}


Factors to convert aticks to pticks \hypertarget{struct__WCT_o5}{
\index{_WCT@{\_\-WCT}!pticks@{pticks}}
\index{pticks@{pticks}!_WCT@{\_\-WCT}}
\subsubsection[pticks]{\setlength{\rightskip}{0pt plus 5cm}unsigned int \hyperlink{struct__WCT_o5}{\_\-WCT::pticks}}}
\label{struct__WCT_o5}


The corresponding number of processor ticks \hypertarget{struct__WCT_o2}{
\index{_WCT@{\_\-WCT}!ptime@{ptime}}
\index{ptime@{ptime}!_WCT@{\_\-WCT}}
\subsubsection[ptime]{\setlength{\rightskip}{0pt plus 5cm}unsigned int \hyperlink{struct__WCT_o2}{\_\-WCT::ptime}}}
\label{struct__WCT_o2}


Value of the lower 32 bits of the processor clock at the time strobe \hypertarget{struct__WCT_o0}{
\index{_WCT@{\_\-WCT}!pTOa@{pTOa}}
\index{pTOa@{pTOa}!_WCT@{\_\-WCT}}
\subsubsection[pTOa]{\setlength{\rightskip}{0pt plus 5cm}\hyperlink{struct__LSU__factors}{LSU\_\-factors} \hyperlink{struct__WCT_o0}{\_\-WCT::p\-TOa}}}
\label{struct__WCT_o0}


Factors to convert pticks to aticks 

The documentation for this struct was generated from the following file:\begin{CompactItemize}
\item 
\hyperlink{WCT__pvtdefs_8h_8vx-xxx-xxx}{WCT\_\-pvtdefs.h.vx-xxx-xxx}\end{CompactItemize}
