\hypertarget{struct____BFcellHeader}{
\section{\_\-\_\-BFcell\-Header Struct Reference}
\label{struct____BFcellHeader}\index{__BFcellHeader@{\_\-\_\-BFcellHeader}}
}
layout of a control cell header  


{\tt \#include $<$latp.h$>$}

\subsection*{Data Fields}
\begin{CompactItemize}
\item 
unsigned short \hyperlink{struct____BFcellHeader_o0}{parity}:1
\item 
unsigned short \hyperlink{struct____BFcellHeader_o1}{source}:6
\item 
unsigned short \hyperlink{struct____BFcellHeader_o2}{proto}: 2
\item 
unsigned short \hyperlink{struct____BFcellHeader_o3}{dest}: 6
\item 
unsigned short \hyperlink{struct____BFcellHeader_o4}{resp}: 1
\end{CompactItemize}


\subsection{Detailed Description}
layout of a control cell header 



\subsection{Field Documentation}
\hypertarget{struct____BFcellHeader_o3}{
\index{__BFcellHeader@{\_\-\_\-BFcell\-Header}!dest@{dest}}
\index{dest@{dest}!__BFcellHeader@{\_\-\_\-BFcell\-Header}}
\subsubsection[dest]{\setlength{\rightskip}{0pt plus 5cm}unsigned short \hyperlink{struct____BFcellHeader_o3}{\_\-\_\-BFcell\-Header::dest}}}
\label{struct____BFcellHeader_o3}


6 bit LAT destination address \hypertarget{struct____BFcellHeader_o0}{
\index{__BFcellHeader@{\_\-\_\-BFcell\-Header}!parity@{parity}}
\index{parity@{parity}!__BFcellHeader@{\_\-\_\-BFcell\-Header}}
\subsubsection[parity]{\setlength{\rightskip}{0pt plus 5cm}unsigned short \hyperlink{struct____BFcellHeader_o0}{\_\-\_\-BFcell\-Header::parity}}}
\label{struct____BFcellHeader_o0}


odd partiy of the header \hypertarget{struct____BFcellHeader_o2}{
\index{__BFcellHeader@{\_\-\_\-BFcell\-Header}!proto@{proto}}
\index{proto@{proto}!__BFcellHeader@{\_\-\_\-BFcell\-Header}}
\subsubsection[proto]{\setlength{\rightskip}{0pt plus 5cm}unsigned short \hyperlink{struct____BFcellHeader_o2}{\_\-\_\-BFcell\-Header::proto}}}
\label{struct____BFcellHeader_o2}


2 bit LATp protocol -- not used by LATp, for client use \hypertarget{struct____BFcellHeader_o4}{
\index{__BFcellHeader@{\_\-\_\-BFcell\-Header}!resp@{resp}}
\index{resp@{resp}!__BFcellHeader@{\_\-\_\-BFcell\-Header}}
\subsubsection[resp]{\setlength{\rightskip}{0pt plus 5cm}unsigned short \hyperlink{struct____BFcellHeader_o4}{\_\-\_\-BFcell\-Header::resp}}}
\label{struct____BFcellHeader_o4}


Boolean, does packet expect a response \hypertarget{struct____BFcellHeader_o1}{
\index{__BFcellHeader@{\_\-\_\-BFcell\-Header}!source@{source}}
\index{source@{source}!__BFcellHeader@{\_\-\_\-BFcell\-Header}}
\subsubsection[source]{\setlength{\rightskip}{0pt plus 5cm}unsigned short \hyperlink{struct____BFcellHeader_o1}{\_\-\_\-BFcell\-Header::source}}}
\label{struct____BFcellHeader_o1}


6 bit LAT source address 

The documentation for this struct was generated from the following file:\begin{CompactItemize}
\item 
\hyperlink{latp_8h}{latp.h}\end{CompactItemize}
