\hypertarget{struct__gtem}{
\section{\_\-gtem Struct Reference}
\label{struct__gtem}\index{_gtem@{\_\-gtem}}
}
struct containing base parameters for the TEM and mini GLT  


{\tt \#include $<$gt\_\-p.h$>$}

\subsection*{Data Fields}
\begin{CompactItemize}
\item 
gnat\-Handle \hyperlink{struct__gtem_o0}{m\_\-gh}
\item 
xbrd\-Handle \hyperlink{struct__gtem_o1}{m\_\-gx}
\item 
unsigned short \hyperlink{struct__gtem_o2}{m\_\-invert\-Cmd\-String\-Parity}
\item 
unsigned short \hyperlink{struct__gtem_o3}{m\_\-invert\-Access\-Desc\-Parity}
\item 
unsigned short \hyperlink{struct__gtem_o4}{m\_\-invert\-Cmd\-Payload\-Parity}
\item 
unsigned short \hyperlink{struct__gtem_o5}{m\_\-AB}
\item 
unsigned int \hyperlink{struct__gtem_o6}{m\_\-int\-Connect}
\end{CompactItemize}


\subsection{Detailed Description}
struct containing base parameters for the TEM and mini GLT 

\_\-gtem is a {\em sub-class\/} of the \_\-gnat struct. 



\subsection{Field Documentation}
\hypertarget{struct__gtem_o5}{
\index{_gtem@{\_\-gtem}!m_AB@{m\_\-AB}}
\index{m_AB@{m\_\-AB}!_gtem@{\_\-gtem}}
\subsubsection[m\_\-AB]{\setlength{\rightskip}{0pt plus 5cm}unsigned short \hyperlink{struct__gtem_o5}{\_\-gtem::m\_\-AB}}}
\label{struct__gtem_o5}


A/B select indicator for command, response \& reset lines \hypertarget{struct__gtem_o0}{
\index{_gtem@{\_\-gtem}!m_gh@{m\_\-gh}}
\index{m_gh@{m\_\-gh}!_gtem@{\_\-gtem}}
\subsubsection[m\_\-gh]{\setlength{\rightskip}{0pt plus 5cm}gnat\-Handle \hyperlink{struct__gtem_o0}{\_\-gtem::m\_\-gh}}}
\label{struct__gtem_o0}


handle to GNAT COMM Board \hypertarget{struct__gtem_o1}{
\index{_gtem@{\_\-gtem}!m_gx@{m\_\-gx}}
\index{m_gx@{m\_\-gx}!_gtem@{\_\-gtem}}
\subsubsection[m\_\-gx]{\setlength{\rightskip}{0pt plus 5cm}xbrd\-Handle \hyperlink{struct__gtem_o1}{\_\-gtem::m\_\-gx}}}
\label{struct__gtem_o1}


handle to GNAT VME XBRD Board \hypertarget{struct__gtem_o6}{
\index{_gtem@{\_\-gtem}!m_intConnect@{m\_\-intConnect}}
\index{m_intConnect@{m\_\-intConnect}!_gtem@{\_\-gtem}}
\subsubsection[m\_\-intConnect]{\setlength{\rightskip}{0pt plus 5cm}unsigned int \hyperlink{struct__gtem_o6}{\_\-gtem::m\_\-int\-Connect}}}
\label{struct__gtem_o6}


Has interrupt been connected ? \hypertarget{struct__gtem_o3}{
\index{_gtem@{\_\-gtem}!m_invertAccessDescParity@{m\_\-invertAccessDescParity}}
\index{m_invertAccessDescParity@{m\_\-invertAccessDescParity}!_gtem@{\_\-gtem}}
\subsubsection[m\_\-invertAccessDescParity]{\setlength{\rightskip}{0pt plus 5cm}unsigned short \hyperlink{struct__gtem_o3}{\_\-gtem::m\_\-invert\-Access\-Desc\-Parity}}}
\label{struct__gtem_o3}


XOR-ed into access descriptor parity -- for testing parity errors \hypertarget{struct__gtem_o4}{
\index{_gtem@{\_\-gtem}!m_invertCmdPayloadParity@{m\_\-invertCmdPayloadParity}}
\index{m_invertCmdPayloadParity@{m\_\-invertCmdPayloadParity}!_gtem@{\_\-gtem}}
\subsubsection[m\_\-invertCmdPayloadParity]{\setlength{\rightskip}{0pt plus 5cm}unsigned short \hyperlink{struct__gtem_o4}{\_\-gtem::m\_\-invert\-Cmd\-Payload\-Parity}}}
\label{struct__gtem_o4}


XOR-ed into command payload parity -- for testing parity errors \hypertarget{struct__gtem_o2}{
\index{_gtem@{\_\-gtem}!m_invertCmdStringParity@{m\_\-invertCmdStringParity}}
\index{m_invertCmdStringParity@{m\_\-invertCmdStringParity}!_gtem@{\_\-gtem}}
\subsubsection[m\_\-invertCmdStringParity]{\setlength{\rightskip}{0pt plus 5cm}unsigned short \hyperlink{struct__gtem_o2}{\_\-gtem::m\_\-invert\-Cmd\-String\-Parity}}}
\label{struct__gtem_o2}


XOR-ed into command string prefix parity -- for testing parity errors 

The documentation for this struct was generated from the following file:\begin{CompactItemize}
\item 
\hyperlink{gt__p_8h}{gt\_\-p.h}\end{CompactItemize}
